HIGH LEVEL STOP LIGHT RELAY LOCATION. Pontiac Sunbird 1985

For 1990-2009 cars

# HIGH LEVEL STOP LIGHT RELAY LOCATION

1985 J2000, SUNBIRD, GRAND AM, BONNEVILLE & GRAND PRIX

The Electrical Troubleshooting Manual does not list the location of the high level stop light relays. The two (2) relays are located in the trunk above the left hand wheel well. Please note this information for future reference.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.