BAT. RUNDOWN INTERIOR LIGHTS REMAIN ON (REPLACE SWITCH). Pontiac Sunbird 1993

For 1990-2009 cars

# BAT. RUNDOWN INTERIOR LIGHTS REMAIN ON (REPLACE SWITCH)

REVISED: 05/09/95

THIS BULLETIN IS BEING REVISED TO CORRECT PARTS INFORMATION FOR THE J CAR. PLEASE DISCARD BULLETIN 438101 (GROUP REFERENCE 8 - CHASSIS/ BODY ELECTRICAL). *********************************************************************

REVISION: 09/18/95

THIS BULLETIN IS BEING REVISED TO UPDATE THE CORRECTION PROCEDURE AND PARTS AND WARRANTY INFORMATION. PLEASE DISCARD BULLETIN 43-81-01A (SECTION 8 - CHASSIS/BODY ELECTRICAL). *********************************************************************

#### SUBJECT: BATTERY RUNDOWN/INTERIOR LIGHTS REMAIN ON (DIAGNOSTIC CHECK/REPLACE DOOR HANDLE SWITCH)

#### MODELS: 1992-94 CHEVROLET CAVALIER 1994 CHEVROLET CORSICA, BERETTA 1992-94 PONTIAC SUNBIRD

#### CONDITION:

SOME OWNERS MAY EXPERIENCE INTERIOR LIGHTS STAYING "ON" AFTER ALL DOORS ARE CLOSED AND AFTER THE MULTI-FUNCTION ALARM MODULE'S INADVERTENT LIGHTING FUNCTION HAS TIMED OUT, CAUSING BATTERY RUNDOWN. IN THE CORSICA/BERETTA, THE MULTI-FUNCTION ALARM MODULE WILL AUTOMATICALLY TURN OFF THE INTERIOR LIGHTS AFTER 20 MINUTES. THE CAVALIER AND SUNBIRD'S INTERIOR LIGHTS WILL CONTINUE TO LIGHT INDEFINITELY.

#### CAUSE:

THE LH AND/OR RH FRONT DOOR HANDLE SWITCH(ES) MAY BE PROVIDING A RESISTIVE PATH TO GROUND WHICH MAY CAUSE THE MULTI-FUNCTION ALARM MODULE TO SENSE THAT THE DOOR(S) ARE FALSELY OPEN.

#### CORRECTION:

FOLLOW THE DIAGNOSTIC PROCEDURE AS LISTED BELOW. IF A RESISTANCE OTHER THAN THE SPECIFIED VALUE REGISTERS DURING TESTING, REPLACE THE MALFUNCTIONING DOOR HANDLE SWITCH, (SEE P/N CHART BELOW). CONTINUE THROUGH THE ENTIRE TEST TO CHECK THAT BOTH THE RH AND LH DOOR HANDLE SWITCHES ARE FUNCTIONING PROPERLY.

1. DISCONNECT THE MULTI-FUNCTION ALARM MODULE.

2. WITH THE LH FRONT DOOR OPEN, MEASURE THE RESISTANCE FROM: TERM "J" TO TERM "P" (J CAR) CONN C1, TERM "H" TO CONN C2, TERM "E" (L CAR) RESISTANCE SHOULD BE BETWEEN 0 - 0.5 OHMS.

3. WITH THE LH FRONT DOOR CLOSED, MEASURE THE RESISTANCE FROM: TERM "J" TO TERM "P" (J CAR) CONN C1, TERM "H" TO CONN C2, TERM "E" (L-CAR) RESISTANCE SHOULD BE > 30 MEGA OHMS.

4. WITH THE RH FRONT DOOR OPEN, MEASURE THE RESISTANCE FROM: TERM "K" TO TERM "P" (J CAR) CONN C1, TERM "G" TO CONN C2, TERM "E" (L-CAR) RESISTANCE SHOULD BE BETWEEN 0 - 0.5 OHMS.

5. WITH THE RH FRONT DOOR CLOSED, MEASURE THE RESISTANCE FROM: TERM "K" TO TERM "P" (J CAR) CONN C1, TERM "G" TO CONN C2, TERM "E" (L-CAR) RESISTANCE SHOULD BE > 30 MEGA OHMS.

#### PARTS INFORMATION:

ALL PARTS ARE FOUND IN GROUP 10.470 -- LOCK ASM F/RH OR LH

#### IMPORTANT: THE DOOR HANDLE SWITCHES ARE PART OF THE FRONT SIDE DOOR LOCK ASSEMBLY.

PART NUMBER CARLINE DOOR SIDE COUPE/SEDAN =========== ======= ========= ===========

16630698 J CAR RH COUPE & SEDAN 16630699 J CAR LH COUPE & SEDAN 16630804 L CAR RH COUPE 16630805 L CAR LH COUPE 16630802 L CAR RH SEDAN 16630803 L CAR LH SEDAN

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T3422 (FOR DIAGNOSTIC CHECK) LABOR TIME: 0.4 (J-CAR) 0.3 (L-CAR)

LABOR OPERATION NUMBER: B4260 (RH) (DOOR HANDLE SWITCH REPLACEMENT) B4261 (LH) ( " " " " ) LABOR TIME: 1.0 HR (J CAR) 0.4 HR (L CAR, 2 DOOR) 0.8 HR (L CAR, 4 DOOR)

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.