RUPTURED INLET HEATER HOSE NEW HOSE P/N AVAILABLE. Pontiac T1000 1987

For 1990-2009 cars

# RUPTURED INLET HEATER HOSE NEW HOSE P/N AVAILABLE

RUPTURED INLET HEATER HOSE

#### VEHICLES AFFECTED: 1985 THRU 1987 "T 9, CAR WITH 1.6L ENGINE -----------------

Customer comments have been received on Ruptured Inlet Heater Hose. To repair this condition a new hose, P/N 10065741, with improved material specifications has been released for service.

Use applicable labour operations for hose replacement.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.