For 1990-2009 cars

# SMU-SECTIONS 3F, 3F4, OR 5 8A-47, 9J - LOC. OF AIRBAG FUS

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTIONS 3F, 3F4 OR 5, 8A-47, 9J - LOCATION OF "AIR BAG" FUSE

#### MODELS: 1994-95 CHEVROLET LUMINA MINIVAN 1994-95 OLDSMOBILE SILHOUETTE 1994-95 PONTIAC TRANS SPORT

THE SIR "AIR BAG" FUSE IS LOCATED BEHIND THE PASSENGER SIDE OF THE I/P LOWER EXTENSION HOUSING (I/P CENTER CONSOLE) (SEE FIGURE 1). THE "AIR BAG" FUSE IS AN IN-LINE FUSE LOCATED 10 INCHES DOWN FROM THE DERM CONNECTOR, TAPED TO THE YELLOW PORTION OF THE WIRE HARNESS (SEE FIGURE 2).

FIGURES: 2 ATTACHMENTS: 0 FIGURE 1 - FRONT VIEW I/P LOWER EXTENSION HOUSING "AIR BAG" FUSE LOCATION - ART PTR53621701

FIGURE 2 - REAR VIEW I/P LOWER EXTENSION HOUSING "AIR BAG" FUSE LOCATION - ART PTR53621702

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.