For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Auxiliary Video Module (AVM) | Overhead console, Left side of video screen. | Entertainment Component Views | Entertainment Connector End Views
CD Player | In the center of the IP floor console. | -- | --
Data Link Connector (DLC) | Below the steering column, on the bottom of the knee bolster. | Entertainment Component Views | Data Link Communications Connector End Views in Wiring Systems
Door Speaker (LF/RF) | Inside front door. | -- | --
Fuse Block | Right side of instrument panel, in Right Front door opening. | Entertainment Component Views | --
Headlamp and I/P Lamp Dimmer Switch | Left of instrument cluster. | -- | --
Inflatable Restraint Steering Wheel Module | In the center of the steering wheel, includes the horn switches. | SIR Component Views in SIR | SIR Connector End Views in SIR
Inflatable Restraint Steering Wheel Module Coil | In the center of the steering wheel, behind the inflatable restraint steering wheel module. | SIR Component Views in SIR | SIR Connector End Views in SIR
Interface Module (IM) | Inside overhead console, Left corner. | Entertainment Component Views | Entertainment Connector End Views
Powertrain Control Module (PCM) | In the engine compartment, secured in the air cleaner assembly. | Engine Controls Component Views in Engine Controls - 3.4L | Powertrain Control Module Connector End Views in Engine Controls - 3.4L
Radio | Center of instrument panel. | -- | --
Radio Control Switches | On the left and right sides of the inflatable restraint steering wheel module. | -- | --
Radio Liftgate Speakers, (LH/RH) | Inside liftgate. | -- | --
Rear Seat Audio (RSA) Control (4-Door) | In the left 2nd row seat armrest. | -- | --
Rear Seat Audio (RSA) Control (5-Door) | Overhead console, Right corner. | Entertainment Component Views | Entertainment Connector End Views
Second Seat Audio (SSA) Control | Overhead console, Right side of video screen. | Entertainment Component Views | Entertainment Connector End Views
Tape Retract Module (TRM) | Underneath Left side instrument panel, near Left side of the Data Link Connector (DLC), taped to the VCP harness. | Entertainment Component Views | Entertainment Connector End Views
Third Seat Audio (TSA) Control | Right quarter trim panel, next to the third row right seat. | Entertainment Component Views | Entertainment Connector End Views
Underhood Accessory Wiring Junction Block | In the engine compartment, at the front of the right wheelhouse, above the battery. | -- | --
Video Cassette Player (VCP) | Front floor console. | Entertainment Component Views | --
Video Entertainment System (VES) Relay | Underneath Left side instrument panel, near Right side of the Data Link Connector (DLC), taped to the VCP harness. | Entertainment Component Views | Entertainment Connector End Views
Video Screen - Liquid Crystal Display (LCD) | In the center of the overhead console. | Entertainment Component Views | --
Windshield Antenna | Within the windshield. | -- | --
C203 | Instrument panel wiring harness to Left side of body wiring harness, Left side of steering column, below P101. | -- | --
C205 | Instrument panel wiring harness to the steering wheel radio control wiring harness, mounted to the left side of the steering column near the base. | -- | --
C290 | In the antenna coaxial cable wiring harness to the antenna coaxial cable wiring harness, behind the IP compartment. | -- | --
C302 | Body wiring harness to the right front side door wiring harness, behind the right kick panel. | -- | --
C303 | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake. | -- | --
C308 | Body wiring harness to the dome lamp wiring harness, inside the right B-pillar, behind the lower trim. | -- | --
C326 | Inside overhead console, in front of the video display bracket assembly, tucked underneath the headliner. | Harness Routing Views in Wiring Systems | Entertainment Connector End Views
C328 | Inside overhead console, in front of the video display bracket assembly, tucked underneath the headliner. | Harness Routing Views in Wiring Systems | Entertainment Connector End Views
C396 | In the antenna coaxial cable wiring harness to the window radio antenna lead, above the roof headliner, at the center of the windshield. | Harness Routing Views in Wiring Systems | Entertainment Connector End Views
C402 | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate. | Harness Routing Views in Wiring Systems | Entertainment Connector End Views
G200 | Right side of instrument panel, secured on underside of cross vehicle beam, to the left of the heater-A/C vent. | -- | --
G201 | Left side of instrument panel, secured on underside of cross vehicle beam, above park brake assembly. | -- | --
G210 | Left side of the front floor console bracket. | Harness Routing Views in Wiring Systems | --
G390 | Antenna coaxial cable secured with clamp, grounding the coaxial shield to the top of the windshield frame, at the right of the mirror. | Harness Routing Views in Wiring Systems | --
P100 | Right side of bulkhead, Left of right strut tower. | -- | --
P406 | Between Right side of liftgate and roof. | -- | --
P500 | Between the left A-pillar and the left front door. | -- | --
P600 | Between the right A-pillar and the right front door. | -- | --
S202 | Instrument panel wiring harness, Right side of the instrument panel, approximately 21 cm (8 in) from radio breakout. | -- | --
S203 | Instrument panel wiring harness, Right side of the instrument panel, approximately 9 cm (4 in) from radio breakout. | -- | --
S223 | Instrument panel wiring harness, Left side of instrument panel, approximately 6 cm (2 in) from radio and rear window wiper/washer multi-function switch breakout. | -- | --
S227 | Instrument panel wiring harness, center of instrument panel, approximately 4 cm (2 in) from security indicator lamp breakout. | -- | --
S230 | Instrument panel wiring harness, Right side of instrument panel, approximately 4 cm (2 in) from radio breakout. | -- | --
S242 | Instrument panel wiring harness, Left side of instrument panel, approximately 14 cm (6 in) from radio and rear window wiper/washer multi-function switch breakout. | -- | --
S247 | Instrument panel wiring harness, center of instrument panel, approximately 31 cm (12 in) from radio. | -- | --
S290 | Video Cassette Player (VCP) wiring harness, next to the Video Entertainment System (VES) relay. | Harness Routing Views in Wiring Systems | --
S291 | Video Cassette Player (VCP) wiring harness, next to the Video Entertainment System (VES) relay. | Harness Routing Views in Wiring Systems | --
S292 | Video Cassette Player (VCP) wiring harness, approximately 30 cm (12 in) Right side of the VES relay. | Harness Routing Views in Wiring Systems | --
S293 | Instrument panel wiring harness, on radio wiring harness breakout, near radio harness connector C1. | Harness Routing Views in Wiring Systems | --
S316 | Body wiring harness, front of Right B-pillar, approximately 34 cm (13 in) from the inflatable restraint sensing and diagnostic module breakout. | -- | --
S320 | Body wiring harness, near base of Right B-pillar, approximately 33 cm (13 in) forward of Right door lock switch plate (pillar mounted, plunger) breakout. | -- | --
S331 | Body wiring harness, front of Left B-pillar, approximately 59 cm (23 in) from G301 breakout. | -- | --