For 1990-2009 cars

# TECH-1 GM 88-92 BRAKE CARTRIDGE EXCHANGE PROGRAM

GM 88-92 BRAKE CARTRIDGE Subject: (TKO3030B) EXCHANGE PROGRAM

#### Models 1988-1992 SUNBIRD, GRAND AM, Affected: GRAND PRIX, SAFARI WAGON AND TRANS SPORT MODELS

This is your opportunity to receive an important update for your Tech 1 from the General Motors Service Technology Group (GM STG). GM STG is offering several enhancements to the GM 88-92 Brake Cartridge (TKO3030B) through a Cartridge Exchange Program. You received this cartridge, designated as essential by Pontiac last fall. We strongly encourage your participation in the Cartridge Exchange Program to receive the following enhancements.

#### Enhancements:

------------ Corrections to all conditions that necessitated the "Important Notice" that accompanied the original cartridge.

Enhanced display of trouble codes when diagnosing 1991-92 Bonneville body vehicles with Teves ABS or TCS systems.

Improved Delco Moraine ABS VI system tests. The updated cartridge will correctly signal the brake motors immediately after termination of the Battery and Motor Tests. It will also improve the Motor Test sequence.

#### Cartridge Exchange Program:

Dealerships that received the Tech 1 GM 88-92 Brake Cartridge (TKO3030B) should exchange it for a revised cartridge (TKO3030C). Follow the instructions listed below and return the cartridge to GM-STG. Once the cartridge is received, an updated cartridge, containing all of the enhancements, will be sent back to the dealership free of charge.

#### Instructions:

------------ Dealers should have received a similar letter, one (1) padded envelope, one (1) GM-STG address label and one (1) dealership return address form. If you did not receive these items, you may send the 88-92 Brake Cartridge (TKO3030B) as described or call the 1-800 phone number listed below.

Complete the following steps to exchange your Tech 1 GM 88-92 Brake Cartridge for an updated cartridge.

Step 1 Fill in the dealership's name, address and dealer code on the Dealership Return Address Form and insert it into the padded envelope. (IMPORTANT: This step must be completed for the updated cartridge to be returned to the dealership.)

Step 2 Locate your Tech 1 GM 88-92 Brake Cartridge (TKO3030B) and insert it into the padded envelope. IMPORTANT: only the affected cartridge should be returned. Accompanying cables, manual and adapters in the kit are not affected and should not be returned with the cartridge.

Step 3 Peel the backing from the GM-STG address label and adhere it to the front of the padded envelope. The address should read:

Service Technology Group Attention: Mr. R. Davalos C/0 Vetronix Corporation 2030 Alameda Padre Serra, Suite 113 Santa Barbara, CA 93103

Step 4 Seal the padded envelope, affix the appropriate postage and mail it to the above address as labeled. (PLEASE NOTE: The sooner the cartridge is received, the sooner the updated cartridge will be returned.)

The updated cartridge will be shipped second day freight after the original GM 88-92 Brake Cartridge has been received by GM-STG. This Cartridge Exchange Program will be in effect through May 15, 1992. Any questions can be directed to the toll free Techline Customer Support Center at 1-800-828-6860. Press "2" for service and then "2" again for Tech 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.