For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
Generator Front Brace to Engine Nut | 25 | 18 | --
Generator Front Brace to Generator Bolt | 50 | 37 | --
Generator Lower Pivot Bolt | 50 | 37 | --
Generator Lower Pivot Nut | 50 | 37 | --
Generator Brace to Manifold Bolt | 25 | 18 | --
Generator Rear Brace to the Rear of Generator Bolt | 25 | 18 | --
Battery Ground (Negative) Cable Bolt | 15 | 11 | --
Battery (Positive) Cable Bolt | 15 | 11 | --
Battery Hold Down Bolt | 18 | 13 | --
Battery Tray Bolts | 10 | 89
Solenoid Battery and Field Terminal Nuts | 10 | -- | 89
Solenoid S Terminal Nuts | 3 | -- | 27
Spark Plugs | 20 | 15 | --
Starter Motor Bolt | 47 | 35 | --