For 1990-2009 cars

#### Connector C111

Connector Part Information |

• | 12129508

• | 7 Way F Metri-Pack 150 Series (BLACK)

Connector Part Information

• | 12146356

• | 7 Way F Metri-Pack 280 Series Pull-to-Seat (Natural)

Pin | Wire Color | ircuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control | A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve
B | YEL/BLK | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control | B | YEL | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve
C | BRN | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control | C | BLK | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve
D | TAN/BLK | 422 | Torque Converter Clutch Solenoid (TCC SOL) Valve Control | D | 422 | TAN | Torque Converter Clutch Solenoid (TCC SOL) Valve
E | PNK | 1339 | Fused Ignition Feed | E | 1339 | RED | Fused Ignition Feed
F | YEL/BLK | 1227 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal | F | 1227 | BRN | Automatic Transaxle Fluid Temperature (TFT) Sensor
G | BLK/WHT | 452 | Sensor Ground |  | 452 | GRY | Ground