For 1990-2009 cars

The GM Adhesive Caulking Kit P/N 10952983 contains the following items:

• | 2 different primers

• | A urethane adhesive with a nozzle

• | Daubers

• | Instructions with warnings

Use the urethane adhesive caulking kit for the following procedures:

• | Replacement of any urethane adhesive-installed window using the short method

• | Replacement of any urethane adhesive-installed window using the extended method

You may use an equivalent urethane adhesive system if the system meets GM Specification GM 3651M. Always follow the system manufacturer's instructions for application, handling and curing.