For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control Systems | Body Control System Connector End Views in Body Control Systems
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Interior Lamp and Multifunction Switch | Center in front of the roof headliner | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Left Front Door Lock (Actuator Motor) | In the left front door, part of the door lock module | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Front Door Lock Cylinder Switch | Inside the left front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Front Door Lock Switch | In the left front door armrest | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Front Window Regulator Motor | Inside the left front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Front Window Switch | In the armrest of the left front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Door Lock Switch Plate (Door Mounted, Plunger) | Mounted to the lower, front end of the left rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Door Lock Switch Plate (Pillar Mounted, Striker) | Mounted to the lower, rear side of the left B-pillar | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Mirror Motor Pack | In the left outside rearview mirror | Power Door Systems Component Views | Power Door Systems Connector End Views
Left Outside Rearview Mirror | Mounted to the left front door | -- | --
Left Rear Quarter Window Actuator | Rear part of the left rear quarter window, on the left D-pillar | Power Door Systems Component Views | Power Door Systems Connector End Views
Liftgate Lock (Actuator Motor) | Part of the liftgate lock assembly, inside the liftgate, below the license plate | Wiper/Washer Component Views in Wipers/Washer Systems | Power Door Systems Connector End Views
Liftgate Lock Cylinder Switch | Inside the liftgate, above the license lamps | Stationary Windows Component Views in Stationary Windows | Power Door Systems Connector End Views
Outside Rearview Mirror Remote Control Switch | Mounted to the top front left front door armrest panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Power Sliding Door On/Off Switch | Part of the interior lamp and multifunction switch, in front of the roof headliner | Lighting Systems Component Views in Lighting Systems | --
Power Sliding Door Detent Switch | Inside the right rear door, mounted to the rear of the door | Power Door Systems Component Views | --
Power Sliding Door Open/Close Switch | Part of the interior lamp and multifunction switch, in front of the roof headliner | Lighting Systems Component Views in Lighting Systems | --
Power Sliding Door Unlatch Actuator | Inside the right rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Rear Quarter Window Switch | Part of the interior lamp and multifunction switch, front of the roof headliner | Engine Controls Component Views in Engine Controls | --
Rear Side Door Actuator Control Module | Part of the rear side door actuator motor, right quarter panel, above the wheelhouse | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Actuator Motor | Right quarter panel, above the wheelhouse | -- | --
Rear Sliding Door Alarm | Attached to the rear side door actuator motor, right quarter panel | Power Door Systems Component Views | --
Remote Control Door Lock Receiver (RCDLR) | Behind the center of the IP, underside of the IP trim, near the windshield defrost vent | Keyless Entry Component Views in Keyless Entry | Keyless Entry Connector End Views in Keyless Entry
Right Front Door Lock (Actuator Motor) | In the right door, part of the door lock module | Power Door Systems Component Views | Power Door Systems Connector End Views
Right Front Door Lock Cylinder Switch | Inside the right front door, near the door handle | Power Door Systems Component Views | Power Door Systems Connector End Views
Right Front Door Lock Switch | In the right front door armrest | Power Door Systems Component Views | Power Door Systems Connector End Views
Right Front Window Regulator Motor | Inside right front door | -- | Power Door Systems Connector End Views
Right Front Window Switch | Inside the armrest of the right front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Right Door Lock Switch Plate (Door Mounted, Plunger) | Mounted to the lower, front end of the right rear side door | Power Door Systems Component Views | Power Door Systems Connector End Views
Right Door Lock Switch Plate (Pillar Mounted, Striker) | Mounted to the lower, rear side of the right B-pillar | Power Door Systems Component Views | Power Door Systems Connector End Views
Right Mirror Motor Pack | In the right outside rearview mirror | -- | Power Door Systems Connector End Views
Right Outside Rearview Mirror | Mounted to the right door | -- | --
Right Rear Quarter Window Actuator | Rear part of the right rear quarter window, on the right D-pillar | -- | Power Door Systems Connector End Views
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Transmission/ Transaxle | Engine Controls Connector End Views in Engine Controls
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C301 (10 cavities) | Body wiring harness to the left side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C304 (10 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C308 (23 cavities) | Body wiring harness to the dome lamp wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C401 (4 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C403 (3 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G302 | Secured near the base of the right B-pillar | Harness Routing Views in Wiring Systems | --
G401 | Secured to the lower left D-pillar | Harness Routing Views in Wiring Systems | --
G402 | Secured to the lower right D-pillar | -- | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P405 | Between the left side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views in Wiring Systems | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views in Wiring Systems | --
S202 | IP harness, right side of the IP approximately 21 cm (8 in) from the radio breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and the rear widow wiper/washer multifunction switch breakout | -- | --
S227 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S302 | Body harness, right front door approximately 34 cm (13 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S307 | Body harness, right front door approximately 4 cm (2 in) from C302 breakout | -- | --
S311 | Body harness, under the right front door sill approximately 11 cm (4 in) from the C302 breakout | -- | --
S314 | Body harness, under the right front seat approximately 2 cm (1 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S315 | Body harness, under the right front seat approximately 8 cm (3 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S319 | Body harness, under the right front door sill approximately 17 cm (7 in) C302 breakout | -- | --
S323 | Body harness, under the left front seat approximately 7 cm (3 in) from the seat belt switch breakout | -- | --
S324 | Body harness, top/forward area of the left rear wheel well approximately 5 cm (2 in) behind the second oval clamp | -- | --
S326 | Body harness, top/forward area of the left rear wheel well approximately 13 cm (5 in) behind the second oval clamp | -- | --
S327 | Body harness, under the left front seat approximately 13 cm (5 in) from the seat belt switch | -- | --
S328 | Body harness, between the left D-pillar and the wheel well approximately 32 cm (13 in) forward of the G401 breakout | -- | --
S337 | Body harness, rear of the left B-pillar base approximately 8 cm (3 in) from the P401 breakout | -- | --
S390 | Roof harness, overhead console approximately 10 cm (4 in) from the right sunshade lighted vanity mirror breakout | -- | --
S392 | Roof harness, right B-pillar approximately 52 cm (20 in) from G302 | -- | --
S395 | Roof harness, right side of the overhead console approximately 13 cm (5 in) from the G302 breakout | -- | --
S423 | Body harness, left rear of the body approximately 54 cm (20 in) from the C403 breakout | -- | --
S427 | Body harness, left rear of the body approximately 41 cm (16 in) from the C403 breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the door lock cylinder switch breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --
S604 (w/AB5) | Right door harness, right door approximately 10 cm (4 in) from the right window switch breakout | -- | --
S604 (w/o AB5) | Right door harness, between P600 and the right front speaker breaker | -- | --
S817 | Sliding door harness, inside the right rear side door approximately 11 cm (4 in) from the right rear door latch release actuator breakout | -- | --