For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Driver Seat Adjuster Motor Assembly | Under the left front seat | -- | --
Driver Seat Adjuster Switch | Mounted to the right side of the base of the left seat | -- | Power Seat Connector End Views
Forward/Back Motor | Part of the seat adjuster motor assembly, mounted to the base of the front seat | -- | --
Front Height Motor | Part of the seat adjuster motor assembly, mounted to the base of the front seat | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Passenger Seat Adjuster Motor Assembly | Under the right front seat | -- | --
Passenger Seat Adjuster Switch | Mounted to the side of the base of the right front seat | -- | Power Seat Connector End Views
Rear Height Motor | Part of the seat adjuster motor assembly, mounted to the base of the front seat | -- | --
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in WIring Systems
C313 (2 cavities) | Body wiring harness to the driver seat adjuster switch wiring harness, under the driver seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C314 (2 cavities) | Body wiring harness to the passenger seat adjuster switch wiring harness, under the passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G301 | Secured to the inside of the lower left B-pillar | Harness Routing Views in Wiring Systems | --
S302 | Body harness, right front door approximately 34 cm (13 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S333 | Body harness, front of the left B-pillar approximately 39 cm (15 in) from the G301 breakout | -- | --