For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door conduit. Refer to Front Side Door Conduit Replacement .
4. Remove the front door window belt inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
5. Remove the front door window weather-strip. Refer to Front Side Door Window Weatherstrip Replacement .
6. Remove the front door window. Refer to Front Side Door Window Replacement .
7. Remove the outside rearview mirror. Refer to Power Mirror Replacement .
8. Remove the front door module. Refer to Front Door Module Replacement .
9. Remove the front door outside handle. Refer to Front Side Door Outside Handle Replacement .
10. Remove the front door lock. Refer to Front Side Door Lock Replacement .
11. Remove the front door window belt outer sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
12. Remove the front door window run channel. Refer to Front Side Door Window Channel Replacement .
13. Remove the front door molding. Refer to Door Body Side Molding Replacement .
14. Remove the front door hinges. Refer to Front Side Door Hinge Replacement .
15. Remove the front door from the body.

### Installation Procedure

1. Install the front door to the body.
2. Install the front door hinges. Refer to Front Side Door Hinge Replacement .
3. Install the front door molding. Refer to Door Body Side Molding Replacement .
4. Install the front door window run channel. Refer to Front Side Door Window Channel Replacement .
5. Install the front door window belt outer sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
6. Install the front door lock. Refer to Front Side Door Lock Replacement .
7. Install the front door outside handle. Refer to Front Side Door Outside Handle Replacement .
8. Install the front door module. Refer to Front Door Module Replacement .
9. Install the outside rearview mirror. Refer to Power Mirror Replacement .
10. Install the front door window. Refer to Front Side Door Window Replacement .
11. Install the front door window weather-strip. Refer to Front Side Door Window Weatherstrip Replacement .
12. Install the front door window belt inner sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
13. Install the front door conduit. Refer to Front Side Door Conduit Replacement .
14. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
15. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
16. Adjust the front door. Refer to Front Side Door Adjustment .