For 1990-2009 cars

# Info - December, 2000 Bulletin Summary

Subject: | December, 2000 Bulletin Summary

Models: | 2001 and Prior Passenger Cars and Trucks

The following list is a summary of all the bulletins that were issued in December, 2000. It is intended to let dealerships quickly review the most current bulletins in order to better service their customers. Dealerships will be receiving this type of summary, published as a bulletin, every month.

Bulletin Title | Vehicles Affected | Bulletin Number
--- | --- | ---
Engine
Engine Preset PTO Speed Returns to Idle (Install Relay) | 1998-2001 Chevrolet and GMC C6-7 Medium Duty Conventional Models With 3126 Caterpillar® Diesel Engine and Allison® Automatic Transmission | 00-06-04-047
Intermittent No Start/No Crank (Replace Ignition and Start Switch Assembly) | 2001 Oldsmobile Aurora; 2000-2001 Pontiac Bonneville | 00-08-49-015
Service Engine Lamp Illuminated with DTC P0410 (Replace Air Injection Reaction (AIR) Pump Relay) | 1999 Oldsmobile Intrigue With 3.5L Engine | 00-06-04-048
Idle Air Control Valve (IACV) Hissing Noise (Replace IACV) | 1999-2000 Chevrolet Cavalier; 1999-2000 Pontiac Sunfire; 1999-2000 Chevrolet and GMC S/T Models (S10, Sonoma) With 2.2L Engine | 00-06-04-053
Various Driveability Symptoms-Malfunction Indicator Lamp (MIL) Illuminates Intermittently, DTCs Set, Engine Will Not Start (Repair Wire(s)) | 1999-2000 Pontiac Grand Prix | 00-06-04-049
Intake Manifold Inspection After Severe Internal Engine Damage | 1995-1999 Cadillac Concours; 1995-2001 Cadillac Eldorado, Seville; 1996-2001 Cadillac DeVille; 1995-2001 Oldsmobile Aurora With 4.0L or 4.6L V8 Engine | 00-06-01-026
Transmissions
High Accelerator Pedal Effort (Replace Throttle Valve Control (TV) Cable) | 1999-2000 Chevrolet Tracker With Automatic Transmission | 00-07-30-023
No Reverse, Second Gear, or Fourth Gear (Replace Reaction Sun Shell) | 1996 Buick Roadmaster; 1996 Cadillac Fleetwood; 1996 Chevrolet Caprice; 1996-1999 Chevrolet Camaro, Corvette; 1996-1999 Pontiac Firebird; 1999 Cadillac Escalad; 1996-1999 Chevrolet and GMC C/K, M/L, S/T and G Models; 1996-1999 Oldsmobile Bravada

With Hydra-Matic 4L60-E Automatic Transmission

00-07-30-022

Steering, Suspension , Tires and Wheels
Rear Suspension Creak/Pop Noise (Install Rear Suspension Support Insulators) | 1997-2001 Chevrolet Malibu; 1997-1999 Oldsmobile Cutlass | 00-03-09-003
Tire Radial Force Variation (RFV) | 2001 and Prior Passenger Cars and Trucks | 00-03-10-006
Body and Accessories
Daytime Running Lamp (DRL) Inoperative | 1999-2001 Chevrolet and GMC C/K Pickup (Silverado and Sierra) and Utility (Tahoe, Suburban, Yukon, Yukon XL) Models | 00-08-42-010
Correct Radio Identification and Usage | 2000 Buick LeSabre | 00-08-44-002A
Theftlock® Indicator | 2001 Pontiac Aztek | 00-08-44-009
Thump/Flutter Type Noise from Lower Rear Window Reveal Molding Area (Install Rear Window Seal) | 2001 Oldsmobile Aurora | 00-08-48-004
HVAC Air Outlet Shut-off Door(s) Close with Blower on High (Install Washer(s)) | 2000 Cadillac DeVille | 00-01-39-001A
Water Runs Out of Front Lower Corners of Rear Hatch When Opened (Install Sealer) | 1998-2001 Chevrolet Camaro; 1998-2001 Pontiac Firebird | 00-08-57-004
Rear Bumper Ends Loose at Wheel Openings (Install New Fasteners) | 1999-2001 Chevrolet Tracker | 00-08-62-004
Creaking Type Sound from Right Rear Wheel Opening Area (Reposition Sheet Metal) | 1999-2001 Chevrolet Tracker (4-door models only) | 99-08-59-002A
General Information
October, 2000 Bulletin Summary | 2001 and Prior Passenger Cars and Trucks | 00-00-89-028
Proper Tire Pressure | 2001 Passenger Cars and Trucks | 00-00-90-002
December, 2000 Labor Time Guide Updates | 1996-2001 Passenger Cars and Trucks | 00-00-89-029
Brakes
ABS Lamp Illuminated, ABS DTC 0281 May be Present (Current or in History) (Adjust Stoplamp Switch) | 1995-2000 Chevrolet and GMC C6-7 Medium Duty Conventional Models; 1995-2000 Chevrolet and GMC B7 Medium Duty School Buses With Hydraulic or Air Antilock Brake Systems | 00-05-25-004
HVAC
Poor Heat with Cold Outside Temperatures at Low Engine RPM (Install Auxiliary Coolant Pump) | 1997-1999 Chevrolet Venture; 1997-1999 Oldsmobile Silhouette; 1997-1999 Pontiac Trans Sport; 1999 Pontiac Montana | 00-01-38-011
HVAC Air Outlet Shut-off Door(s) Close with Blower on High (Install Washer(s)) | 2000 Cadillac DeVille | 00-01-39-001A