For 1990-2009 cars

### Removal Procedure

1. Remove the case extension housing. Refer to Case Extension Replacement .
2. Remove the thrust bearing.
3. Remove the thrust washer.
4. Remove the final drive.
5. Disassemble the final drive. Refer to Transmission/Transaxle/Transfer Case Unit Repair Manual.

### Installation Procedure

1. Assemble the final driver. Refer to Transmission/Transaxle/Transfer Case Unit Repair Manual.
2. Install the final drive.
3. Install the thrust washer.
4. Install the thrust bearing.
5. Install the extension housing. Refer to Case Extension Replacement .
6. Measure the end play. Refer to Transmission/Transaxle/Transfer Case Unit Repair Manual.
7. Adjust the fluid level.
8. Inspect for proper completion of the repairs.
9. Inspect for fluid leaks.