For 1990-2009 cars

Illustration | Tool Number/Description
--- | ---
| EN 48869 Front Crankshaft Oil Seal Installer
| J 5239 Connecting Rod Bolt Guide Set
| J 5825-A Crankshaft Sprocket Remover
| J 5892-D Valve Spring Compressor
| J 7872 Magnetic Base Dial Indicator Set
| J 8001 Dial Indicator
| J 8037 Piston Ring Compressor
| J 8087 Cylinder Bore Gage
| J 8089 Wire Brush
| J 8520 Cam Lift Lobe Indicator
| J 9666 Valve Spring Tester
| J 21882 Oil Suction Pipe Installer
| J 22144 Oil Inlet Tube Installer
| J 22794 Spark Plug Port Adapter
| J 23600-B Belt Tension Gauge
| J 24086-C Piston Pin Remover and Installer Set
| J 24270 Cylinder Bore Ridge Reamer
| J 24420-B Crankshaft Balancer Remover
| J 25087-C Oil Pressure Tester and Pump Primer
| J 28428-E High Intensity Black Light
| J 28467-6A Lift Hook Bracket
| J 28467-7A Lift Hook
| J 28467-8A Swivel Lift Hook
| J 28467-34 Lift Hook Wing Nut
| J 28467-90 Engine Support Fixture Adapters
| J 28467-360 Engine Support Fixture
| J 28467-500 Engine Support Fixture
| J 29113 Crankshaft Balancer Installer
| J 33049 Camshaft Bearing Remover and Installer
| J 34686 Crankshaft Rear Oil Seal Installer
| J 35667-A Cylinder Leakage Tester
| J 36462 Engine Support Adapter Leg
| J 36660-A Electronic Torque/Angle Meter
| J 37377 J 37378 J 37379 Valve Guide Reamers
| J 38606 Valve Spring Compressor
| J 38612 Crankshaft Sprocket Installer
| J 38722 Compression Gauge
| J 39344 Harmonic Balancer Installer
| J 39505 Torque Wrench Adapter
| J 41131 Engine Tilt Strap
| J 41816 Crankshaft Balancer Remover