For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Wiring Junction Block Bolt | 10 N·m | 89 lb in
Battery Ground (Negative) Cable Nut to the Transaxle Stud | 25 N·m | 18 lb ft
Battery Ground (Negative) Bolt to the Inner Fender | 5 N·m | 44 lb in
Battery Ground (Negative) Terminal Bolt | 16 N·m | 12 lb ft
Battery Hold-Down Retainer Bolt | 25 N·m | 18 lb ft
Battery (Positive) Terminal Bolt | 16 N·m | 12 lb ft
Battery Tray Bolt | 10 N·m | 89 lb in
Generator - Delphi CS-144 (KG9)

- Battery (Positive) Lead BAT Nut (Generator output BAT Terminal)

25 N·m

18 lb ft

- Generator Bolt (Pivot Bolt)

50 N·m

37 lb ft

- Generator Bracket Bolt

50 N·m

37 lb ft

- Generator Brush Holder Bolt

2.5 N·m

22 lb ft

- Generator Capacitor/Rectifier Bridge Bolt

2.5 N·m

22 lb ft

- Generator Front Brace Bolt

50 N·m

37 lb ft

- Generator Front Brace Nut

25 N·m

18 lb ft

- Generator Nut (Pivot Bolt)

50 N·m

37 lb ft

- Generator Rear Brace Bolt

50 N·m

37 lb ft

- Generator Rear Brace Nut

25 N·m

18 lb ft

- Generator Shaft Nut

100 N·m

74 lb ft

- Generator Stator Lead Nut

2.5 N·m

22 lb ft

- Generator Through Bolt

8 N·m

71 lb in

- Insulated Regulator Bolt

2.5 N·m

22 lb ft

Generator - Valeo A13VI+ (K68)

- Battery (Positive) Lead BAT Nut (Generator output BAT Terminal)

15 N·m

11 lb ft

- Generator Bolt (Pivot Bolt)

50 N·m

37 lb ft

- Generator Bracket Bolt

50 N·m

37 lb ft

- Generator Front Brace Bolt

50 N·m

37 lb ft

- Generator Front Brace Nut

25 N·m

18 lb ft

- Generator Nut (Pivot Bolt)

50 N·m

37 lb ft

- Generator Rear Brace Bolt

25 N·m

18 lb ft

- Generator Rear Brace Nut

25 N·m

18 lb ft

- Generator Rear Cover Nut

2 N·m

18 lb in

- Generator Regulator/Brush Holder Nut

3 N·m

27 lb in

- Generator Regulator Terminal Bolt

2 N·m

18 lb in

- Generator Rotor Shaft Drive End Nut

70 N·m

52 lb ft

Spark Plug | 15 N·m | 11 lb ft
Starter Bolt | 47 N·m | 35 lb ft
Starter Solenoid BAT Terminal Nut | 10 N·m | 89 lb in
Starter Solenoid S Terminal Nut | 3 N·m | 27 lb in