For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Armrest Screws | 3 N·m | 26 lb ft
Bearing Bushing Screw | 2 N·m | 18 lb in
Cone Adjuster Bolt (Body Side) | 10 N·m | 89 lb in
Front Door Lock Module Screws | 10 N·m | 89 lb in
Front Door Lock Striker Screws | 25 N·m | 18 lb ft
Front Door Outside Handle Screws | 10 N·m | 89 lb in
Front Door Window Run Channel Screws | 10 N·m | 89 lb in
Front Quarter Window Hinge Stud Nuts | 10 N·m | 89 lb in
Front Quarter Window Latch Screws | 10 N·m | 89 lb in
Outside Rearview Mirror Motor Screws | 10 N·m | 89 lb in
Outside Rearview Mirror Nuts | 10 N·m | 89 lb in
Power Rear Quarter Window Actuator Screws | 10 N·m | 89 lb in
Power Sliding Door Actuator Motor Bolts | 10 N·m | 89 lb in
Power Sliding Door Actuator Motor Nuts | 10 N·m | 89 lb in
Power Sliding Door Latch Detent Switch Retaining Screws | .9 N·m | 8.5 lb in
Power Sliding Door Latch Release Actuator Screws | 10 N·m | 89 lb in
Rear Quarter Window Hinge Stud Nuts | 10 N·m | 89 lb in
Rear Quarter Window Latch Screws | 10 N·m | 89 lb in
Sliding Door Center Roller Bracket (Door Side) Bolts | 25 N·m | 18 lb ft
Sliding Door Center Track Bracket Screws | 10 N·m | 89 lb in
Sliding Door Center Track Cover Front Screw | 2 N·m | 18 lb in
Sliding Door Center Track Cover Rear Screw | 10 N·m | 89 lb in
Sliding Door Center Track Screws | 10 N·m | 89 lb in
Sliding Door Center Track Screw or Stud | 10 N·m | 89 lb in
Sliding Door Lock Actuator Screws | 10 N·m | 89 lb in
Sliding Door Locating Pin Screws | 10 N·m | 89 lb in
Sliding Door Locating Pocket Screws | 10 N·m | 89 lb in
Sliding Door Lock Screws | 10 N·m | 89 lb in
Sliding Door Lower Roller Bracket Bolts | 10 N·m | 89 lb in
Sliding Door Catch with Reinforcement Channel Bolt | 25 N·m | 18 lb ft
Sliding Door Outside Handle Nuts | 12 N·m | 106 lb in
Sliding Door Striker Screws | 10 N·m | 89 lb in
Sliding Door Swing Out Window Hinge Stud Nuts | 25 N·m | 18 lb ft
Sliding Door Swing Out Window Latch Screws | 10 N·m | 89 lb in
Sliding Door Upper Roller Bracket Bolts | 10 N·m | 89 lb in
Sliding Door Upper Track Screws | 10 N·m | 89 lb in
Upper and Lower Body Side Hinge Bolts | 33 N·m | 24 lb ft
Upper and Lower Door Side Hinge Bolts | 33 N·m | 24 lb ft