For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the radio for correct operation. Does the radio turn ON and OFF? | -- | Go to Step 3 | Go to Step 2
2 |

1. Service the radio. Refer to Radio Replacement .
2. Inspect the system.

Has the repair been made?

--

Go to Radio/Audio System Check

--

3 |

1. Turn the ignition to the OFF position.
2. Remove the MALL/RADIO/DIC fuse and the RADIO fuse for 1 minute.
3. Reinstall the fuses.
4. Turn the ignition to the RUN position.
5. Turn on the radio.

Does the radio display LOC?

--

Go to Step 2

Go to Radio/Audio System Check