For 1990-2009 cars

1. Remove the coast clutch retainer plate retaining ring (611) with a screwdriver.
2. Remove the coast clutch retainer plate (610).
3. Remove the coast clutch end bearing (608) and the coast one way clutch (609).
4. Remove the coast clutch outer race (607).
5. Remove the rear planetary ring gear flange retaining ring (604) with snap ring pliers.
6. Remove the rear planetary ring gear flange (605) from the rear planetary ring gear (606).