For 1990-2009 cars

1. Install the transmission output speed sensor (74).

Caution: Refer to Fastener Caution in the Preface section.

2. Mount the speed sensor to the case with the 1 speed sensor bolt (75). Tighten the bolt to 5.4 N·m (48 lb in).
3. Install the transmission input speed sensor (76).
4. Mount the speed sensor to the case with the 1 speed sensor bolt (75). Tighten the bolt to 5.4 N·m (48 lb in).