For 1990-2009 cars

### Removal Procedure

1. Remove the inside rear view mirror.
2. Remove the rain sensor cover.
3. Disconnect the wiring harness plug (1).
4. Compress the clamp (2) and pull the mirror downwards to remove.

### Installation Procedure

1. Install the interior rear view mirror.
2. If removed, install the spring catch to the mirror.
3. Replace the mirror and listen for the click.
4. Connect the wiring harness plug.
5. Install the rain sensor cover.