For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Bracket Bolts | 15 N·m | 11 lb ft
Battery Ground Connection Nut | 5 N·m | 44 lb in
Battery Holder Bolts | 7 N·m | 62 lb in
Battery Positive Connection Nut | 5 N·m | 44 lb in
Battery Support Bolts | 10 N·m | 89 lb in
Hydraulic Line Retaining Bolt | 14 N·m | 10 lb ft
Hydraulic Modulator Bolts | 8 N·m | 71 lb in
Hydraulic Modulator Bracket Bolts | 20 N·m | 15 lb ft
Yaw Rate/Acceleration Sensor Nuts | 10 N·m | 89 lb in