For 1990-2009 cars

Caution: Refer to Brake Dust Caution in the Preface section.

1. Remove brake linings. Refer to Front Disc Brake Pads Replacement or Rear Disc Brake Pads Replacement .
2. Measure the remaining brake lining thickness with a caliper (1).
3. Nominal values. Refer to Disc Brake Component Specifications .
4. Install brake pads.
5. Install the brake linings. Refer to Front Disc Brake Pads Replacement or Rear Disc Brake Pads Replacement .