For 1990-2009 cars

Condition | Action
--- | ---
DEFINITION: Noise shifting while sitting still and shifting from neutral to reverse or drive
Engine or transmission mounts |

• | Inspect the engine mounts and the transmission mounts for wear or loose mounting fasteners.

• | Replace any faulty engine or transmission mounts or loose fasteners.

Drive shafts |

• | Inspect the drive shafts for worn components.

• | Replace the drive shaft if worn.