For 1990-2009 cars

### Removal Procedure

1. Open the access panel in the wheel house liner.
2. Remove the turn signal lamp bulbs with the holder.

• | Turn the holder in the direction of the arrow.

• | Remove the holder.

3. Remove the bulb from the holder.

### Installation Procedure

1. Install the bulb in the holder.
2. Install the turn signal lamp bulbs with the holder.
3. Close the access panel.