For 1990-2009 cars

The F17 is a 5 speed manual transmission assembly.

Important: Use only transmission fluid listed within the Lubrication Specifications for this manual transmission assembly. Other lubricants or additives may affect the shift performance.

The F17 5 Speed manual transmission has the following features:

• | First and second gear double coned synchronizer

• | Third, fourth, and fifth gear single coned synchronizer

• | Two shaft design consisting of an input shaft, and main shaft

• | Reverse inhibit feature

• | One piece clutch actuator - no bleed screw

• | Transmission venting system is part of the fill cap

• | First gear ratio is 3.73

• | Second gear ratio is 2.14

• | Third gear ratio is 1.41

• | Fourth gear ratio is 1.12

• | Fifth gear ratio is 0.89

• | Reverse gear ratio is 3.31

• | Final drive ratio is 3.94

• | Vehicle speed sensor (VSS)

The manual transmission shift cables must be adjusted for proper shifter performance.