For 1990-2009 cars

Caution: Storing a jack, a tire, or other equipment in the passenger compartment of the vehicle could cause injury. In a sudden stop or collision, loose equipment could strike someone. Store all these in the proper place.

To store a flat or spare tire and tools, do the following:

1. Jack

2. Wheel Wrench

3. Screwdriver

4. Jack Handle

1. Replace the jack and tools as shown.
2. Place the flat tire face down into the spare tire hub.
3. Turn spare tire hold-down bolt by turning clockwise. Return the foam pad to its original position.
4. Put the load floor back in place.

The compact spare tire is for temporary use only. Replace the compact spare with a full-size tire as soon as possible.