For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Crossmember Bolts | 5 N·m | 44 lb in
Front Window Screws | 4 N·m | 35 lb in
Power Sunroof Motor Bolts | 7 N·m | 62 lb in
Sunroof Bolts - Front and Rear | 4 N·m | 35 lb in
Sunroof Module Assembly Screws | 5 N·m | 44 lb in
Sunroof Motor Bolts | 4 N·m | 35 lb in
Sunroof Window Screws | 4 N·m | 35 lb in
Sunshade Motor Bolts | 4 N·m | 35 lb in
Sunshade to Rail Bolts | 2.5 N·m | 22 lb in
Wheelhouse Liner Bolts | 2.5 N·m | 22 lb in
Wind Deflector Clamp Bolts | 2.5 N·m | 22 lb in
Wind Deflector Swing-Out Arm Bolts | 2 N·m | 18 lb in