For 1990-2009 cars

Figure 1: |

#### Right Front of the Engine

(1) | Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust
(2) | Engine Oil Pressure (EOP) Switch

Figure 2: |

#### Top of the Engine

(1) | Fuel Injector 1
(2) | Fuel Injector 2
(3) | Engine Control Module (ECM)
(4) | Fuel Injector 3
(5) | Fuel Injector 4
(6) | Battery
(7) | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Figure 3: |

#### Left Side of the Engine

(1) | Ignition Control Module (ICM)
(2) | Camshaft Position (CMP) Sensor - Intake
(3) | Engine Coolant Temperature (ECT) Sensor
(4) | Heated Oxygen Sensor (HO2S) 1, Connector
(5) | Camshaft Position (CMP) Sensor - Exhaust
(6) | G104

Figure 4: |

#### Automatic Transmission (MNF)

(1) | Park/Neutral Position (PNP) Switch
(2) | X100
(3) | X113
(4) | Automatic Transmission Output Shaft Speed (OSS) Sensor
(5) | Automatic Transmission Input Shaft Speed (ISS) Sensor

Figure 5: |

#### Right Rear of the Engine

(1) | X110
(2) | Camshaft Position (CMP) Actuator Solenoid Valve - Intake
(3) | Throttle Body
(4) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve