For 1990-2009 cars

### Removal Procedure

1. Remove the wiring harness from the brake fluid reservoir.
2. Disconnect the wiring harness plug (1) from the brake fluid level sensor (2).
3. Remove the brake fluid level sensor from the brake fluid reservoir.

Press out carefully with a screwdriver.

### Installation Procedure

1. Insert the brake fluid level sensor in the brake fluid reservoir and clip in position.
2. Connect the wiring harness plug to the brake fluid level sensor.
3. Connect the wiring harness on at the brake fluid reservoir.