For 1990-2009 cars

# Front Radiator Grille Emblem/Nameplate Delaminating or Discoloring (Install New Emblem)

Subject: | Front Radiator Grille Emblem/Nameplate Delaminating or Discoloring (Install New Emblem)

Models: | 2008 Saturn Astra

### Condition

Some customers may comment that the red color from the radiator grille emblem is discolored or delaminating.

### Cause

This condition may be due to the reflective material on the back side of the emblem wearing through due to contact to with the radiator grill housing standoffs.

### Correction

1. Remove the radiator grille emblem/nameplate following SI.
2. Remove just the upper chrome portion of the grille.
3. Cover both of the radiator grille standoffs with squeak reduction tape. Refer to the arrows in the illustration above

The squeak reduction tape can be purchased locally or online (*Kent Anti-Squeak Film Tape KT13512 or *3M™ Squeak Reduction Tape 06356).

4. Install a new emblem in the grille.
5. Reinstall the chrome portion of the grille and reinstall the grille.

*We believe these sources and their products to be reliable. There may be additional manufacturers of such products. General Motors does not endorse, indicate any preference for or assume any responsibility for the products from these firms or for any such items which may be available from other sources.

### Parts Information

Part Number | Description
--- | ---
94706491 | Plate, Rad Grl He Bkg (Red) Backing Emblem

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
B9856* | Apply Tape to Radiator Grille | 0.3 hr
*This is a unique labor operation for bulletin use only. It will not be published in the Labor Time Guide.