For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Column Integration Module (CIM) Bolt | 15 N·m | 11 lb ft
Engine Electrical Center Bolt | 6 N·m | 53 lb in
Ground Connection Bolt | 5 N·m | 44 lb in
Lower Steering Column Paneling Screws | 1 N·m | 9 lb in
Steering Wheel Bolt | 30 N·m | 22 lb ft
Voltage Supply Nut | 7 N·m | 62 lb in
Wiring Harness to Positive Terminal Bolt | 10 N·m | 89 lb in