For 1990-2009 cars

Condition | Action
--- | ---
DEFINITION: Engine stalls when slowing down
Transmission Control Module (TCM) |

• | Inspect for proper calibration of the TCM.

• | Re-cal TCM.

• | Replace TCM if faulty.

Transmission oil cooler pipe |

• | Inspect transmission oil cooler system for restricted or kinked lines.

• | Replace faulty oil cooler line.

Valve body (39) | Replace valve body (39).