For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Strip Panel Bolts | 3 N·m | 26 lb in
Brake Pedal Bearing Support Bolts | 20 N·m | 15 lb ft
Center Trim Panel Bolts | 2.5 N·m | 22 lb in
Clutch Pedal Bearing Support Bolts | 20 N·m | 15 lb ft
Driver Side Knee Bolster Bolts | 3 N·m | 26 lb in
Driver Side Knee Bolster Lower Bracket Bolts | 2.5 N·m | 22 lb in
Front Floor Console Bolts | 2.5 N·m | 22 lb in
Ground Cable Bolts | 5 N·m | 44 lb in
Ignition Lock Panel Screws | 2.5 N·m | 22 lb in
Information Display Bolts | 3 N·m | 26 lb in
Instrument Cluster Bolts | 3 N·m | 26 lb in
Instrument Panel Compartment Bolt | 4 N·m | 35 lb in
Instrument Panel Compartment Door Bolt | 2.5 N·m | 22 lb in
Instrument Panel Retainer Bolts - Left Side | 13 N·m | 113 lb in
Instrument Panel Tie Bar Bolts | 20 N·m | 15 lb ft
Instrument Panel Tie Bar Center Bracket Bolts | 13 N·m | 113 lb in
Instrument Panel Trim Bolt - Lower | 6 N·m | 53 lb in
Instrument Panel Trim Bolt - Upper | 13 N·m | 113 lb in
Selector Lever Cover Bolts | 2.5 N·m | 22 lb in
Shift Lever Bezel Bolts | 2.5 N·m | 22 lb in
Steering Column (CIM Module) Bolts | 3.8 N·m | 34 lb in
Steering Column Panel Bolts - Lower | 1 N·m | 9 lb in
Steering Column Panel Bolts - Upper | 2.5 N·m | 22 lb in
Steering Column Panel Screws - Upper | 0.5 N·m | 8 lb in
Steering Wheel Bolt | 30 N·m | 22 lb ft