For 1990-2009 cars

Connector 1: | 1/2-3/4 Shift Solenoid (SS) Valve (MNF)
Connector 2: | 2/3 Shift Solenoid (SS) Valve (MNF)
Connector 3: | Accessory Power Outlet
Connector 4: | A/C Compressor Clutch (C60)
Connector 5: | A/C Refrigerant Pressure Sensor (C60)
Connector 6: | Accelerator Pedal Position (APP) Sensor
Connector 7: | Air Temperature Actuator
Connector 8: | Ambient Air Temperature Sensor 1
Connector 9: | Ambient Air Temperature Sensor 2
Connector 10: | Antenna
Connector 11: | Automatic Transmisssion Input Shaft Speed (ISS) Sensor (MNF)
Connector 12: | Automatic Transmisssion Fluid Temperature (TFT) Sensor (MNF)
Connector 13: | Automatic Transmisssion Output Shaft Speed (OSS) Sensor (MNF)
Connector 14: | Automatic Transmission Shift Lever Position Indicator (MNF)
Connector 15: | Backup Lamp Switch (M25)
Connector 16: | Barometric Pressure (BARO) Sensor
Connector 17: | Battery
Connector 18: | Blower Motor
Connector 19: | Blower Motor Resistor Assembly
Connector 20: | Brake Booster Pump Motor
Connector 21: | Brake Fluid Level Switch
Connector 22: | Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust
Connector 23: | Camshaft Position (CMP) Actuator Solenoid Valve - Intake
Connector 24: | Camshaft Position (CMP) Sensor - Exhaust
Connector 25: | Camshaft Position (CMP) Sensor - Intake
Connector 26: | Cargo Lamp
Connector 27: | Cellular Telephone Microphone
Connector 28: | Center High Mounted Stop Lamp (CHMSL)
Connector 29: | Clutch Pedal Position (CPP) Switch (M25)
Connector 30: | Courtesy/Reading Lamps - 2nd Row
Connector 31: | Crankshaft Position (CKP) Sensor
Connector 32: | Cruise Control Clutch Pedal Release Switch (M25)
Connector 33: | Data Link Connector (DLC)
Connector 34: | Dome/Reading Lamp - Front
Connector 35: | Door Lock - Driver
Connector 36: | Door Lock - Left Rear
Connector 37: | Door Lock - Passenger
Connector 38: | Door Lock Relay
Connector 39: | Door Lock - Right Rear
Connector 40: | Door Unlock Relay
Connector 41: | Driver Information Center (DIC)
Connector 42: | Electronic Brake Control Module (EBCM)
Connector 43: | Engine Control Module (ECM) X1
Connector 44: | Engine Control Module (ECM) X2
Connector 45: | Engine Control Module (ECM) X3
Connector 46: | Engine Coolant Level Switch
Connector 47: | Engine Coolant Temperature (ECT) Sensor
Connector 48: | Engine Cooling Fan (MNF with C41 or M25)
Connector 49: | Engine Cooling Fan - Left (MNF with C60)
Connector 50: | Engine Cooling Fan - Right (MNF with C60)
Connector 51: | Engine Oil Level (EOL) Switch
Connector 52: | Engine Oil Pressure (EOP) Switch
Connector 53: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 54: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
Connector 55: | Fog Lamp - Left Front (T96)
Connector 56: | Fog Lamp - Right Front (T96)
Connector 57: | Fuel Door Release Actuator
Connector 58: | Fuel Injector 1
Connector 59: | Fuel Injector 2
Connector 60: | Fuel Injector 3
Connector 61: | Fuel Injector 4
Connector 62: | Fuel Pump and Sender Assembly
Connector 63: | Fuel Tank Pressure (FTP) Sensor
Connector 64: | Generator - X1
Connector 65: | Generator - X2
Connector 66: | Headlamp - Left High Beam Solenoid
Connector 67: | Headlamp - Left Low Beam
Connector 68: | Headlamp - Right High Beam Solenoid
Connector 69: | Headlamp - Right Low Beam
Connector 70: | Headlamp and Panel Dimmer Switch
Connector 71: | Heated Oxygen Sensor (HO2S) 1
Connector 72: | Heated Oxygen Sensor (HO2S) 2
Connector 73: | Heated Seat Element - Driver Cushion (KA1)
Connector 74: | Heated Seat Element - Passenger Cushion (KA1)
Connector 75: | Hood Ajar Switch
Connector 76: | Horn
Connector 77: | HVAC Control Module, X1
Connector 78: | HVAC Control Module, X2
Connector 79: | I/P Compartment - Lamp
Connector 80: | Ignition Control Module (ICM)
Connector 81: | Inflatable Restraints Front End Sensor - Left
Connector 82: | Inflatable Restraint Front End Sensor - Right
Connector 83: | Inflatable Restraint Front Passenger Presence System (PPS) Module
Connector 84: | Inflatable Restraint I/P Module - X1
Connector 85: | Inflatable Restraint I/P Module - X2
Connector 86: | Inflatable Restraint Steering Wheel Module - X1
Connector 87: | Inflatable Restraint Steering Wheel Module - X2
Connector 88: | Inflatable Restraint Roof Rail Module - Left
Connector 89: | Inflatable Restraint Roof Rail Module - Right
Connector 90: | Inflatable Restraint Sensing and Diagnostic Module (SDM) - X1
Connector 91: | Inflatable Restraint Sensing and Diagnostic Module (SDM) - X2
Connector 92: | Inflatable Restraint Side Impact Sensor (SIS) - Left
Connector 93: | Inflatable Restraint Side Impact Sensor (SIS) - Right
Connector 94: | Inflatable Restraint Steering Wheel Module Coil
Connector 95: | Inside Rearview Mirror (ISRVM)
Connector 96: | Instrument Panel Cluster (IPC)
Connector 97: | Intake Manifold Tuning (IMT) Solenoid Valve
Connector 98: | Intake Manifold Tuning Valve (IMTV) Sensor
Connector 99: | K50 Relay (C3U)
Connector 100: | K93 Relay (MNF)
Connector 101: | Knock Sensor (KS)
Connector 102: | License Lamp - Left
Connector 103: | License Lamp - Right
Connector 104: | Liftgate Latch Assembly
Connector 105: | Liftgate Release Switch
Connector 106: | Mass Air Flow (MAF) / Intake Air Temperature (IAT) sensor
Connector 107: | Mode Actuator
Connector 108: | Multifunction Switch - I/P
Connector 109: | Neutral Control Solenoid Valve (MNF)
Connector 110: | Outside Rearview Mirror - Driver
Connector 111: | Outside Rearview Mirror - Passenger
Connector 112: | Park Brake Switch
Connector 113: | Park/Neutral Position (PNP) Switch (MNF)
Connector 114: | Position Lamp - Left
Connector 115: | Position Lamp - Right
Connector 116: | Power Steering Control Module (PSCM) - X1 (NS2/NR1)
Connector 117: | Power Steering Control Module (PSCM) - X2
Connector 118: | Pressure Control (PC) Solenoid Valve (MNF)
Connector 119: | Radio - X1
Connector 120: | Rear Window Defogger Grid - X1
Connector 121: | Rear Window Defogger Grid - X2
Connector 122: | Rear Window Wiper Motor
Connector 123: | Recirculation Actuator
Connector 124: | Repeater Lamp - Left Front
Connector 125: | Repeater Lamp - Right Front
Connector 126: | Seat Position Sensor - Passenger
Connector 127: | Side Marker Lamp - Left Front
Connector 128: | Side Marker Lamp - Left Rear
Connector 129: | Side Marker Lamp - Right Front
Connector 130: | Side Marker Lamp - Right Rear
Connector 131: | Speaker - Center I/P
Connector 132: | Speaker - Left Front Tweeter (U65)
Connector 133: | Speaker - Left Front
Connector 134: | Speaker - Left Rear
Connector 135: | Speaker - Right Front
Connector 136: | Speaker - Right Front Tweeter (U65)
Connector 137: | Speaker - Right Rear
Connector 138: | Starter - X1
Connector 139: | Starter - X2
Connector 140: | Steering Wheel Control Switch - Left
Connector 141: | Steering Wheel Control Switch - Right
Connector 142: | Steering Column Control Module
Connector 143: | Stop Lamp Switch
Connector 144: | Sunroof Control Module (C3U)
Connector 145: | Sunroof Shade Module (C3U)
Connector 146: | Sunroof Shade Switch (C3U)
Connector 147: | Sunroof Switch (C3U)
Connector 148: | Sunshade - Left
Connector 149: | Sunshade - Right
Connector 150: | Tail Lamp - Left
Connector 151: | Tail Lamp - Right
Connector 152: | Throttle Body
Connector 153: | Tire Pressure Module
Connector 154: | Torque Converter Clutch (TCC) Solenoid Valve (MNF)
Connector 155: | Transmission Control Module (TCM) (MNF)
Connector 156: | Vehicle Communication Interface Module (VCIM) Battery
Connector 157: | Vehicle Communications Interface Module (VCIM) - Left - X1
Connector 158: | Vehicle Communications Interface Module (VCIM) - Left - X2
Connector 159: | Vehicle Communications Interface Module (VCIM) - Left - X4
Connector 160: | Vehicle Communications Interface Module (VCIM) - Left - X5
Connector 161: | Vehicle Communications Interface Module (VCIM) - Left - X6
Connector 162: | Vehicle Communications Interface Module (VCIM) - Right
Connector 163: | Wheel Speed Sensor (WSS) - Left Front
Connector 164: | Wheel Speed Sensor (WSS) - Left Rear
Connector 165: | Wheel Speed Sensor (WSS) - Right Front
Connector 166: | Wheel Speed Sensor (WSS) - Right Rear
Connector 167: | Window Motor - Driver
Connector 168: | Window Motor - Left Rear (5 Door)
Connector 169: | Window Motor - Passenger
Connector 170: | Window Motor - Right Rear (5 Door)
Connector 171: | Window Switch - Driver
Connector 172: | Window Switch - Left Rear (5 Door)
Connector 173: | Window Switch - Passenger
Connector 174: | Window Switch - Right Rear (5 Door)
Connector 175: | Windshield Outside Moisture Sensor
Connector 176: | Windshield Washer Fluid Level Switch
Connector 177: | Windshield Washer Fluid Pump
Connector 178: | Windshield Wiper Motor
Connector 179: | Winter Mode Switch (MNF)
Connector 180: | Yaw and Lateral Accelerometer Sensor (FX3)

### 1/2-3/4 Shift Solenoid (SS) Valve (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### 1/2-3/4 Shift Solenoid (SS) Valve (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Low Reference
B | BK | 1526 | Shift Solenoid Supply Voltage 2

### 2/3 Shift Solenoid (SS) Valve (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### 2/3 Shift Solenoid (SS) Valve (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Low Reference
B | WH | 1525 | Shift Solenoid Supply Voltage 1

### Accessory Power Outlet

#### Connector Part Information

- OEM: 926522-1
- Service: 9198842
- Description: 2-Way F Positive Lock Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service Connector Assembly - 9198842
- Release Tool/Test Probe: N/A

#### Accessory Power Outlet

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.5 BN | 1650 | Ground
2 | 1.5 RD | 502 | Battery Positive Voltage

### A/C Compressor Clutch (C60)

#### Connector Part Information

- OEM: 2880-4147-0773
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### A/C Compressor Clutch (C60)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1.5 BN/RD | 1250 | Ground
B | 1 BK/WH | 59 | A/C Compressor Clutch Supply Voltage

### A/C Refrigerant Pressure Sensor (C60)

#### Connector Part Information

- OEM: 30432421
- Service: Service by Harness - See Part Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### A/C Refrigerant Pressure Sensor (C60)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/BK | 5514 | Low Reference
2 | 0.5 BK/WH | 2700 | 5 Volt Reference 1
3 | 0.5 GN | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 6-929264-1
- Service: 89046653
- Description: 6-Way F MT2 Housing (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 89046653
- Release Tool/Test Probe: N/A

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/YE | 1274 | 5 Volt Reference 2
2 | 0.5 BK/RD | 1164 | 5 Volt Reference 1
3 | 0.5 WH/YE | 1161 | Accelerator Pedal Position Signal 1
4 | 0.5 BN/RD | 1271 | Low Reference
5 | 0.5 BN/WH | 1272 | Low Reference
6 | 0.5 WH/GN | 1162 | Accelerator Pedal Position Signal 2

### Air Temperature Actuator

#### Connector Part Information

- OEM:1355082-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F MQS Series, (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Air Temperature Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/BK | -- | 8V Reference
2 | GY | -- | Air Temperature Actuator Position Signal
3 | BK | -- | Low Reference
4 | -- | -- | Not Used
5 | RD | -- | Air Temperature Actuator Motor Control B
6 | WH | -- | Air Temperature Actuator Motor Control A

### Ambient Air Temperature Sensor 1

#### Connector Part Information

- OEM: 1452680-2
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Ambient Air Temperature Sensor 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 636 | Outside Ambient Air Temperature Sensor Signal
2 | 0.5 BU/BN | 61 | Low Reference

### Ambient Air Temperature Sensor 2

#### Connector Part Information

- OEM: 1452680-2
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Ambient Air Temperature Sensor 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 636 | Outside Ambient Air Temperature Sensor Signal
2 | 0.5 BU/BN | 61 | Low Reference

### Antenna

#### Connector Part Information

- OEM: 1355648-1
- Service: Service by Harness - See Part Catalog
- Description: 4-Way M 64 MQS Series, Sealed (D-BU)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Antenna

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.35 COAX | 5173 | Antenna Radio Screen
2 | -- | -- | Not Used
3 | 0.35 COAX | 6797 | GSM Antenna Screen
4 | 0.35 COAX | 5175 | Antenna Navigation Screen

### Automatic Transmisssion Input Shaft Speed (ISS) Sensor (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Automatic Transmisssion Input Shaft Speed (ISS) Sensor (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GN | 1231 | Low Reference
B | YE/BK | 1230 | Transmission Speed Sensor Signal

### Automatic Transmisssion Fluid Temperature (TFT) Sensor (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Automatic Transmisssion Fluid Temperature (TFT) Sensor (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | OG | 586 | Low Reference
B | OG | 585 | Transmission Oil Temperature Sensor Signal

### Automatic Transmisssion Output Shaft Speed (OSS) Sensor (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Automatic Transmisssion Output Shaft Speed (OSS) Sensor (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | 401 | Low Reference
B | YE | 400 | Vehicle Speed Sensor Signal

### Automatic Transmission Shift Lever Position Indicator (MNF)

#### Connector Part Information

- OEM: 962321-1
- Service: Service by Harness - See Part Catalog
- Description: 12-Way F 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Automatic Transmission Shift Lever Position Indicator (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BN | 2150 | Ground
3-4 | -- | -- | Not Used
5 | 0.5 BK | 539 | Run/Crank Ignition 1 Voltage
6 | -- | -- | Not Used
7 | 0.5 GY/YE | 1382 | LED Dimming Signal
8 | 0.5 WH | 771 | Transmission Position Switch Bit 1 Signal
9 | 0.5 GN | 772 | Transmission Position Switch Bit 2 Signal
10 | 0.5 GY | 773 | Transmission Position Switch Bit 3 Signal
11 | 0.5 WH/YE | 1371 | Transmission Position Switch Bit 4 Signal
12 | -- | -- | Not Used

### Backup Lamp Switch (M25)

#### Connector Part Information

- OEM: ID401561
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Backup Lamp Switch (M25)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.75 BN | 650 | Ground
B | 0.75 WH/BK | 5007 | Reverse Switch Signal

### Barometric Pressure (BARO) Sensor

#### Connector Part Information

- OEM: 15397338
- Service: Service by Harness - See Part Catalog
- Description: 3-Way F 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Barometric Pressure (BARO) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/BN | 474 | 5 Volt Reference 1
2 | 0.5 GN/BK | 6014 | Low Reference
3 | 0.5 GN/BN | 5266 | Ambient Air Pressure Sensor Signal

### Battery

#### Connector Part Information

- OEM: KBP25-10
- Service: Service by Harness - See Part Catalog
- Description: 1-Way F

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Battery

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | 50 BK | 1 | Unfused Battery Positive Voltage
25 RD | 1 | Unfused Battery Positive Voltage

### Blower Motor

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Blower Motor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | -- | Blower Motor Supply Voltage
B | BK | -- | Ground

### Blower Motor Resistor Assembly

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 7-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Blower Motor Resistor Assembly

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Medium 1 Blower Motor Control
2 | BU | -- | Medium 2 Blower Motor Control
3 | BK | 1850 | Ground
4 | OG | -- | Low Blower Motor Control
5 | GN | -- | High Blower Motor Control
6 | PU | -- | Blower Motor Supply Voltage
7 | BK | -- | Ground

### Brake Booster Pump Motor

#### Connector Part Information

- OEM: 7283-5575-10
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F YESC/USCAR Class III Series, Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Brake Booster Pump Motor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 BK | 7448 | Brake Booster Pump Supply Voltage
2 | 2.5 BN | 1350 | Ground

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 1452680-2
- Service: 93186673
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service Connector Assembly - 93186673
- Release Tool/Test Probe: N/A

#### Brake Fluid Level Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 1350 | Ground
2 | 0.5 BN/RD | 333 | Brake Fluid Level Sensor Signal

### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust

#### Connector Part Information

- OEM: 248556-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BN/YE | 5284 | CMP Actuator Solenoid Control - Exhaust
2 | 0.75 RD/BU | 5291 | Ignition Voltage

### Camshaft Position (CMP) Actuator Solenoid Valve - Intake

#### Connector Part Information

- OEM: 248556-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Camshaft Position (CMP) Actuator Solenoid Valve - Intake

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BN/YE | 5272 | CMP Actuator Solenoid Control - Intake
2 | 0.75 RD/BU | 5291 | Ignition Voltage

### Camshaft Position (CMP) Sensor - Exhaust

#### Connector Part Information

- OEM: 2FW 3-45
- Service: 19179748
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service Connector Assembly - 19179748
- Release Tool/Test Probe: N/A

#### Camshaft Position (CMP) Sensor - Exhaust

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 633 | Camshaft Position Sensor Signal - Exhaust
2 | 0.5 BN/YE | 632 | Low Reference
3 | 0.5 BK/WH | 474 | 5 Volt Reference 1

### Camshaft Position (CMP) Sensor - Intake

#### Connector Part Information

- OEM: 2FW 3-45
- Service: 19179748
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 19179748
- Release Tool/Test Probe: N/A

#### Camshaft Position (CMP) Sensor - Intake

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 633 | Camshaft Position Sensor Signal - Intake
2 | 0.5 BN/YE | 632 | Low Reference
3 | 0.5 BK/WH | 474 | 5 Volt Reference 1

### Cargo Lamp

#### Connector Part Information

- OEM: F2-14
- Service: 19178170
- Description: 2-Way F 6.3 Faston Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 19178170
- Release Tool/Test Probe: N/A

#### Cargo Lamp

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GY/GN | 737 | Trunk Lamp Control
2 | 0.5 BN | 2350 | Ground

### Cellular Telephone Microphone

#### Connector Part Information

- OEM: ID696728
- Service: 12085481
- Description: 2-Way F Metri-Pack 150 Lang Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service Connector Assembly - 12085481
- Release Tool/Test Probe: N/A

#### Cellular Telephone Microphone

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.35 BK | 5193 | Low Reference
B | 0.35 BU/RD | 5191 | Cellular Telephone Microphone Signal

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: 1452140-3
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 2550 | Ground
2 | 0.5 BK/YE | 820 | CHMSL Supply Voltage

### Clutch Pedal Position (CPP) Switch (M25)

#### Connector Part Information

- OEM: 12033711
- Service: 93184057
- Description: 2-Way F Metri-Pack 480 Series (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93184057
- Release Tool/Test Probe: N/A

#### Clutch Pedal Position (CPP) Switch (M25)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 VT | 1935 | CPP Starter Control
B | 0.5 BK | 1039 | ECM Starter Control

### Courtesy/Reading Lamps - 2nd Row

#### Connector Part Information

- OEM: F4-28
- Service: Service by Harness - See Part Catalog
- Description: 4-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Courtesy/Reading Lamps - 2nd Row

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.18 FW | 1550 | Ground (-C3U)
0.18 WH | 1550 | Ground (C3U)
2 | 0.18 FW | 1732 | Inadvertant Power Courtesy Lamp (-C3U)
0.18 GN | 1732 | Inadvertant Power Courtesy Lamp (C3U)
3 | -- | -- | Not Used
4 | 0.18 FW | 157 | Interior Lamp Control (-C3U)
0.18 YE | 157 | Interior Lamp Control (C3U)

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: ZFW 3-45
- Service: 19179748
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 19179748
- Release Tool/Test Probe: N/A

#### Crankshaft Position (CKP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 573 | Crankshaft Position Sensor Signal
2 | 0.5 BN/YE | 574 | Low Reference
3 | 0.5 BK/WH | 474 | 5 Volt Reference 1

### Cruise Control Clutch Pedal Release Switch (M25)

#### Connector Part Information

- OEM: 968943-3
- Service: 93184057
- Description: 4-Way F 64 MQS Series (BN)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93184057
- Release Tool/Test Probe: N/A

#### Cruise Control Clutch Pedal Release Switch (M25)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 BK | 1039 | Run/Crank Ignition 1 Voltage
4 | 0.5 GY | 379 | Cruise Control Clutch Pedal Position Switch Signal

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 15488184
- Service: 19115029
- Description: 16-Way F 1.2 Timer, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Data Link Connector (DLC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
2 | 0.5 BN/VT | 1132 | DLC Class 2 Serial Data
3 | 0.5 GN | 5169 | Mid Speed GMLAN Serial Data (+)
4 | 0.5 BN | 2150 | Ground
5 | 0.5 BN | 2150 | Ground
6 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
7 | 0.5 GN/WH | 377 | Serial Data
8-10 | -- | -- | Not Used
11 | 0.5 WH | 5170 | Mid Speed GMLAN Serial Data (-)
12-13 | -- | -- | Not Used
14 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
15 | -- | -- | Not Used
16 | 0.75 RD | 1442 | Battery Positive Voltage

### Dome/Reading Lamp - Front

#### Connector Part Information

- OEM: ID800092
- Service: 93180710
- Description: 18-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Dome/Reading Lamp - Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | 0.5 BN | 1550 | Ground
6 | 0.5 RD/BU | 1732 | Inadvertant Power Courtesy Lamp
7 | 0.5 GY | 157 | Interior Lamp Control
8-13 | -- | -- | Not Used
14 | 0.5 GY/YE | 1382 | LED Dimming Signal
15-18 | -- | -- | Not Used

### Door Lock - Driver

#### Connector Part Information

- OEM: 1355688-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Door Lock - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
3-5 | -- | -- | Not Used
6 | 0.5 WH/GY | 49 | Driver Door Ajar Switch Signal
7 | 0.5 BN | 1550 | Ground
8 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal
9-10 | -- | -- | Not Used

### Door Lock - Left Rear

#### Connector Part Information

- OEM: 6-1355683-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Door Lock - Left Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
3 | -- | -- | Not Used
4 | 0.5 BN | 2350 | Ground
5 | 0.5 GY | 747 | Left Rear Door Ajar Switch Signal
6 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal

### Door Lock - Passenger

#### Connector Part Information

- OEM: 6-1355688-1
- Service: Service by Harness - See Part Catalog
- Description: 10-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Door Lock - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
3-5 | -- | -- | Not Used
6 | 0.5 GY | 746 | Right Front Door Ajar Switch Signal
7 | 0.5 BN | 2050 | Ground
8 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal
9-10 | -- | -- | Not Used

### Door Lock Relay

#### Connector Part Information

- OEM: 12034003
- Service: 88987189
- Description: 5-Way F Special Metri-Pack 630 Unsealed, Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88987189
- Release Tool/Test Probe: N/A

#### Door Lock Relay

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 RD | 342 | Battery Positive Voltage
2 | 0.5 VT | 7306 | Emergency Door Unlock Control
3 | 1.5 GY/WH | 7305 | Emergency Door Unlock 1 Signal
4 | 1.5 RD | 195 | Door Unlock Control
5 | 1.5 BN | 2350 | Ground

### Door Lock - Right Rear

#### Connector Part Information

- OEM: 6-1355683-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Door Lock - Right Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.75 GY/WH | 7305 | Emergency Door Unlock 2 Signal
3 | -- | -- | Not Used
4 | 0.5 BN | 2350 | Ground
5 | 0.5 GY | 748 | Right Rear Door Ajar Switch Signal
6 | 0.75 WH | 7304 | Emergency Door Unlock 1 Signal

### Door Unlock Relay

#### Connector Part Information

- OEM: 12034003
- Service: 88987189
- Description: 5-Way F Special Metri-Pack 630 Unsealed, Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88987189
- Release Tool/Test Probe: N/A

#### Door Unlock Relay

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 RD | 342 | Battery Positive Voltage
2 | 0.5 VT | 7306 | Emergency Door Unlock Control
3 | 1.5 WH | 7304 | Emergency Door Unlock 2 Signal
4 | 1.5 WH | 194 | Door Lock Control
5 | 2.5 RD | 342 | Battery Positive Voltage

### Driver Information Center (DIC)

#### Connector Part Information

- OEM: 968265-1
- Service: 88988405
- Description: 32-Way F 0.64 Quadlock Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Driver Information Center (DIC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BN | 1750 | Ground
2 | 0.75 BN | 1750 | Ground (UAG)
3 | 0.75 RD | 3140 | Battery Positive Voltage (UAG)
4 | -- | -- | Not Used
5 | 0.75 RD | 3140 | Battery Positive Voltage
6-18 | -- | -- | Not Used
19 | 0.5 WH | 5170 | Mid Speed GMLAN Serial Data (-)
20 | 0.5 GN | 5169 | Mid Speed GMLAN Serial Data (+)
21 | -- | -- | Not Used
22 | 0.5 GN | 5169 | Mid Speed GMLAN Serial Data (+)
23 | 0.5 WH | 5170 | Mid Speed GMLAN Serial Data (-)
24 | -- | -- | Not Used
25 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
26-27 | -- | -- | Not Used
28 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
29-32 | -- | -- | Not Used

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: 1452643-1
- Service: 88988362
- Description: 26-Way F MT2/SPT Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Electronic Brake Control Module (EBCM)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 4 RD | 3240 | Battery Positive Voltage
2 | 0.5 BN/BU | 885 | Low Reference
3 | 0.5 BU | 884 | Wheel Speed Sensor Signal - Left Rear
4 | 0.5 GN/BK | 1338 | Yaw Rate Sensor Signal 2
5 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal - Right Front
6 | 0.5 BN/RD | 833 | Low Reference
7 | -- | -- | Not Used
8 | 0.5 BN/WH | 873 | Low Reference
9 | 0.5 BU/WH | 830 | Wheel Speed Sensor Signal - Left Front
10 | 0.5 GY/BK | 1337 | Yaw Rate Sensor Volt Reference
11 | 0.5 BU/RD | 882 | Wheel Speed Sensor Signal - Right Rear
12 | 0.5 BN/RD | 883 | Low Reference
13 | 4 BN | 1450 | Ground
14 | 4 RD | 3340 | Battery Positive Voltage
15-16 | -- | -- | Not Used
17 | 0.5 BU/BN | 1903 | AAS Wheel Speed Sensor Signal - Left Front
18 | -- | -- | Not Used
19 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
20 | 0.75 BK | 3 | Run/Crank Ignition 1 Voltage
21 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
22 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal
23 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
24 | 0.5 RD | 1202 | Battery Positive Voltage
25 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
26 | 4 BN | 1450 | Ground

### Engine Control Module (ECM) X1

#### Connector Part Information

- OEM: 15368916
- Service: 88956567
- Description: 64-Way F 0.6 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Engine Control Module (ECM) X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/RD | 2121 | Ignition Control 1
2 | 0.5 BU/RD | 2121 | Ignition Control 1
3 | 0.5 YE/VT | 5041 | Intake Manifold Control 1
4 | -- | -- | Not Used
5 | 0.5 BU/YE | 231 | Oil Pressure Switch Signal
6 | 0.5 BK | 808 | Low Reference
7 | 0.5 BU | 5042 | Intake Manifold Tuning Valve Sensor Signal
8 | 0.5 BU | 486 | Throttle Position Sensor Signal 2
9 | 0.5 BU | 485 | Throttle Position Sensor Signal 1
10 | 0.5 GY/BK | 496 | KS Signal
11 | 0.5 BK | 808 | Low Reference
12 | 0.5 BN/GN | 472 | Intake Air Temperature Sensor Signal
13-14 | -- | -- | Not Used
15 | 0.5 BK/WH | 474 | 5 Volt Reference 1
16 | 0.5 BN/YE | 5041 | Low Reference
17 | 0.5 BU/WH | 2122 | Ignition Control 2
18 | 0.5 BU/WH | 2122 | Ignition Control 2
19 | 0.5 BK/BN | 1423 | Heated Oxygen Sensor Heater Low Control Sensor 2
20 | -- | -- | Not Used
21 | 0.5 BU | 633 | Camshaft Position Sensor Signal
22 | 0.5 BU | 633 | Camshaft Position Sensor Signal
23 | 0.5 BN/YE | 1664 | Heated Oxygen Sensor Low Signal Sensor 1
24 | 0.5 BN/YE | 632 | Low Reference
25 | 0.5 BN/YE | 2761 | Low Reference
26 | 0.5 BN/YE | 632 | Low Reference
27 | 0.5 GY/RD | 1716 | KS Signal
28 | 0.5 BK/VT | 469 | Low Reference
29 | 0.5 BN/YE | 1669 | Heated Oxygen Sensor Low Signal Sensor 2
30 | -- | -- | Not Used
31 | 0.5 YE/BK | 581 | Throttle Actuator Control Open
32 | 0.5 BK/WH | 581 | Throttle Actuator Control Open
33 | 0.5 BU/GN | 2123 | Ignition Control 3
34 | 0.5 BU/GN | 2123 | Ignition Control 3
35 | 0.5 BU | 573 | Crankshaft Position Sensor Signal 1
36 | 0.5 BU/WH | 1174 | Oil Level Switch Signal
37-38 | -- | -- | Not Used
39 | 0.5 BN/YE | 574 | Low Reference
40 | 0.5 BN/WH | 2752 | Low Reference
41 | 0.5 BK/WH | 2701 | 5 Volt Reference 2
42 | 0.5 BK/WH | 474 | 5 Volt Reference 1
43 | 0.5 BN/YE | 650 | Low Reference
44 | 0.5 BK | 808 | Low Reference
45 | -- | -- | Not Used
46 | 0.5 BN/WH | 428 | EVAP Canister Purge Solenoid Control
47 | 0.5 BN/WH | 582 | Throttle Actuator Control Close
48 | 0.5 BN/WH | 582 | Throttle Actuator Control Close
49 | 0.5 BU/YE | 2124 | Ignition Control 4
50 | 0.5 BU/YE | 2124 | Ignition Control 4
51-52 | -- | -- | Not Used
53 | 0.5 BU | 1665 | Heated Oxygen Sensor High Signal Sensor 1
54 | 0.5 BU | 1668 | Heated Oxygen Sensor High Signal Sensor 2
55 | 0.75 BN/YE | 5284 | CMP Actuator Solenoid Control Exhaust
56 | 0.75 BN/YE | 5272 | CMP Actuator Solenoid Control Intake
57 | -- | -- | Not Used
58 | 0.75 BK/BN | 676 | Heated Oxygen Sensor Heater High Control Sensor 1
59 | 0.5 GN/WH | 492 | Mass Air Flow Sensor Signal
60 | 0.5 BU/RD | 410 | Engine Coolant Temperature Sensor Signal
61 | 0.5 BN/BK | 1745 | Fuel Injector Control 2
62 | 0.5 BN/VT | 1746 | Fuel Injector Control 3
63 | 0.5 BN/YE | 844 | Fuel Injector Control 4
64 | 0.5 BN/RD | 1744 | Fuel Injector Control 1

### Engine Control Module (ECM) X2

#### Connector Part Information

- OEM: ZFW64-8
- Service: Service by Harness - See Part Catalog
- Description: 64-Way F Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Engine Control Module (ECM) X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 998 | MIL Control
2-5 | -- | -- | Not Used
6 | 0.5 GN | 2501 | High Speed GMLAN Serial Data (-)
7-9 | -- | -- | Not Used
10 | 0.5 RD/WH | 335 | Low Speed Cooling Fan Relay Control
11 | -- | -- | Not Used
12 | 0.5 BN/PU | 1 | Brake Booster Pump Relay Control
13-15 | -- | -- | Not Used
16 | 0.5 BK/YE | 379 | Cruise Control Clutch Pedal Position Switch Signal
17-22 | -- | -- | Not Used
23 | 0.5 BK/WH | 2700 | 5 Volt Reference 1
24 | 0.5 BK/WH | 1164 | 5 Volt Reference 1
25 | 0.5 BK/WH | 1274 | 5 Volt Reference 2
26 | 0.5 BN | 1271 | Low Reference
27 | 0.5 BN | 1272 | Low Reference
28-29 | -- | -- | Not Used
30 | 0.5 BN/BU | 5514 | Low Reference
31 | 0.75 RD | 5290 | Ignition Voltage
32 | 0.5 RD | 3540 | Battery Positive Voltage
33-34 | -- | -- | Not Used
35 | 0.5 BN/BU | 6014 | Low Reference
36 | 0.5 BN/VT | 61 | Low Reference
37 | -- | -- | Not Used
38 | 0.5 BU | 2500 | High Speed GMLAN Serial Data (+)
39 | 0.5 BN/BU | 251 | Low Reference
40-41 | -- | -- | Not Used
42 | 0.5 BU/YE | 890 | Fuel Tank Pressure Sensor Signal
43 | 0.5 BN/GN | 636 | Outside Ambient Air Temperature Sensor Signal
44 | 0.5 BU | 5266 | Ambient Air Pressure Sensor Signal
45 | 0.5 BK/YE | 848 | Brake Switch Signal
46 | 0.5 BN/YE | 2759 | Low Reference
47 | 0.75 RD | 5290 | Ignition Voltage
48 | 0.5 BN/VT | 1 | Brake Booster Vacuum Pump Control
49 | 0.5 BN/GN | 465 | Fuel Pump Primary Relay Control
50-51 | -- | -- | Not Used
52 | 0.5 BU/WH | 225 | Generator Turn On Signal
53 | 0.5 BK/YE | 1162 | Accelerator Pedal Position Signal 2
54 | 0.5 BK/YE | 1161 | Accelerator Pedal Position Signal 1
55 | 0.5 GN/BU | 30 | Fuel Level Sensor Signal
56 | 0.5 YE/RD | 203 | A/C High Pressure Switch Signal
57 | 0.5 BK/YE | 340 | Stop Lamp Switch Signal
58 | 0.5 BN | 2350 | EVAP Canister Vent Solenoid Control
59 | 0.5 RD/WH | 473 | High Speed Cooling Fan Relay Control
60 | 0.5 BU/BK | 1039 | ECM Starter Control
61 | 0.5 RD/WH | 5267 | Turbo Cooling Fan Relay Control
62 | 0.5 BN/YE | 5069 | Engine Main Relay Coil Control
63 | -- | -- | Not Used
64 | 0.5 BK | 39 | Run/Crank Ignition 1 Voltage

### Engine Control Module (ECM) X3

#### Terminal Part Information

- Terminal: 56.3-1
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Engine Control Module (ECM) X3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | 2.5 BN | 650 | Ground

### Engine Coolant Level Switch

#### Connector Part Information

- OEM: 1452680-2
- Service: 93186673
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186673
- Release Tool/Test Probe: N/A

#### Engine Coolant Level Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/GN | 68 | Low Coolant Level Indicator Control
2 | 0.5 BN | 1350 | Ground

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 12162195
- Service: 88987993
- Description: 2-Way F Metri-Pack 150.2 Series, Pull-to-Seat Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88987993
- Release Tool/Test Probe: N/A

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/RD | 410 | Engine Coolant Temperature Sensor Signal
2 | 0.5 BN/YE | 2761 | Low Reference

### Engine Cooling Fan (MNF with C41 or M25)

#### Connector Part Information

- OEM: 15446375
- Service: 93186714
- Description: 3-Way F Ducon 6.3 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186714
- Release Tool/Test Probe: N/A

#### Engine Cooling Fan (MNF with C41 or M25)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 6 BN | 1250 | Ground
B | 6 RD/YE | 409 | Cooling Fan Motor Supply Voltage 1
C | 6 RD/WH | 532 | Cooling Fan Motor Supply Voltage 2

### Engine Cooling Fan - Left (MNF with C60)

#### Connector Part Information

- OEM: 15446375
- Service: 93186714
- Description: 3-Way F Ducon 6.3 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186714
- Release Tool/Test Probe: N/A

#### Engine Cooling Fan - Left (MNF with C60)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 6 BN | 1250 | Ground
B | -- | -- | Not Used
C | 6 RD/YE | 409 | Cooling Fan Motor Supply Voltage 2

### Engine Cooling Fan - Right (MNF with C60)

#### Connector Part Information

- OEM: 15446375
- Service: 93186714
- Description: 3-Way F Ducon 6.3 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186714
- Release Tool/Test Probe: N/A

#### Engine Cooling Fan - Right (MNF with C60)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 6 BN/GN | 504 | Low Reference
B | -- | -- | Not Used
C | 6 RD/WH | 532 | Cooling Fan Motor Supply Voltage 1

### Engine Oil Level (EOL) Switch

#### Connector Part Information

- OEM: 15397337
- Service: 88988744
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assenbly - 88988744
- Release Tool/Test Probe: N/A

#### Engine Oil Level (EOL) Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/WH | 1174 | Oil Level Switch Signal
2 | 0.5 BN/YE | 650 | Ground

### Engine Oil Pressure (EOP) Switch

#### Connector Part Information

- OEM: 12065299
- Service: 12085500
- Description: 1-Way F Metri-Pack 150 Series, Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 12085500
- Release Tool/Test Probe: N/A

#### Engine Oil Pressure (EOP) Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/YE | 231 | Oil Pressure Switch Signal

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 12052637
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 12101858
- Release Tool/Test Probe: N/A

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 RD/BU | 5291 | Ignition Voltage
2 | 0.5 BN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Metri-Pack 150 Series, Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1 BU | 5372 | Ignition Voltage
B | 1 BN | 2350 | EVAP Canister Vent Solenoid Control

### Fog Lamp - Left Front (T96)

#### Connector Part Information

- OEM: ZFW2-10
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Fog Lamp - Left Front (T96)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.5 BN | 1150 | Ground
2 | 1.5 BN/GY | 5061 | Left Front Fog Lamp Supply Voltage

### Fog Lamp - Right Front (T96)

#### Connector Part Information

- OEM: ZFW2-10
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Fog Lamp - Right Front (T96)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.5 BN | 1050 | Ground
2 | 1.5 BN/GN | 5062 | Right Front Fog Lamp Supply Voltage

### Fuel Door Release Actuator

#### Connector Part Information

- OEM: 1452140-3
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Fuel Door Release Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BU/BK | 6801 | Fuel Door Lock Control
2 | 0.75 BU | 6800 | Fuel Door Unlock Control

### Fuel Injector 1

#### Connector Part Information

- OEM: 15397337
- Service: 88988744
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88988744
- Release Tool/Test Probe: N/A

#### Fuel Injector 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 RD/BU | 260 | Fuel Injection Control
2 | 0.5 BN/RD | 1744 | Fuel Injector Control 1

### Fuel Injector 2

#### Connector Part Information

- OEM: 15397337
- Service: 88988744
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88988744
- Release Tool/Test Probe: N/A

#### Fuel Injector 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 RD/BU | 260 | Fuel Injection Control
2 | 0.5 BN/BK | 1745 | Fuel Injector Control 2

### Fuel Injector 3

#### Connector Part Information

- OEM: 15397337
- Service: 88988744
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88988744
- Release Tool/Test Probe: N/A

#### Fuel Injector 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 RD/BU | 260 | Fuel Injection Control
2 | 0.5 BN/VT | 1746 | Fuel Injector Control 3

### Fuel Injector 4

#### Connector Part Information

- OEM: 15397337
- Service: 88988744
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88988744
- Release Tool/Test Probe: N/A

#### Fuel Injector 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 RD/BU | 260 | Fuel Injection Control
2 | 0.5 BN/YE | 844 | Fuel Injector Control 4

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 15326631
- Service: Service by Harness - See Part Catalog
- Description: 4-Way F GT 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Fuel Pump and Sender Assembly

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1.5 BN | 2350 | Ground
B | 0.5 BN/YE | 251 | Low Reference
C | 0.5 GN/BU | 30 | Fuel Level Sensor Signal
D | 1.5 RD/BU | 120 | Fuel Pump Supply Voltage

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 13511996
- Service: Service by Harness - See Part Catalog
- Description: 3-Way F GT 150 Series, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/WH | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.5 BK/GN | 2759 | Low Reference
3 | 0.5 BK/YE | 2709 | 5 Volt Reference 1

### Generator - X1

#### Connector Part Information

- Terminal: S8.4-24
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Generator - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | 16 RD | 1 | Battery Positive Voltage

### Generator - X2

#### Connector Part Information

- OEM: ZFW 2-141
- Service: 88988744
- Description: 2-Way F Junior Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88988744
- Release Tool/Test Probe: N/A

#### Generator - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BU/WH | 225 | Generator Turn On Signal
2 | -- | -- | Not Used

### Headlamp - Left High Beam Solenoid

#### Connector Part Information

- OEM:1-968704-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Headlamp - Left High Beam Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 1150 | Ground
2 | BK | 711 | Left Headlamp High Beam Supply Voltage

### Headlamp - Left Low Beam

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Headlamp - Left Low Beam

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1150 | Ground
B | BK | 712 | Left Headlamp Low Beam Supply Voltage

### Headlamp - Right High Beam Solenoid

#### Connector Part Information

- OEM:1-968704-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Headlamp - Right High Beam Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 1050 | Ground
2 | BK | 311 | Right Headlamp High Beam Supply Voltage

### Headlamp - Right Low Beam

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Headlamp - Right Low Beam

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1050 | Ground
B | BK | 312 | Right Headlamp Low Beam Supply Voltage

### Headlamp and Panel Dimmer Switch

#### Connector Part Information

- OEM: 968473-1
- Service: 93191114
- Description: 12-Way F 64 MQS Series (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93191114
- Release Tool/Test Probe: N/A

#### Headlamp and Panel Dimmer Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 GY/GN | 13 | Headlamp Switch Park Lamp Signal
3 | -- | -- | Not Used
4 | 0.5 GY/VT | 44 | Instrument Panel Lamp Dimmer Switch Signal
5 | 0.5 YE | 1201 | Headlamp Low Beam
6 | 0.5 BN | 1650 | Ground
7 | 0.5 BK | 1039 | Run/Crank Ignition 1 Voltage
8 | 0.5 GY/BU | 192 | Front Fog Lamp Switch Signal (T96)
9-10 | -- | -- | Not Used
11 | 0.5 BN/YE | 1651 | Low Reference
12 | -- | -- | Not Used

### Heated Oxygen Sensor (HO2S) 1

#### Connector Part Information

- OEM: ZMW4-7
- Service: Service by Harness - See Part Catalog
- Description: 4-Way M Sealed (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Heated Oxygen Sensor (HO2S) 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BK/BN | 676 | Heated Oxygen Sensor Heater High Control Sensor 1
2 | 0.5 BU | 1665 | Heated Oxygen Sensor High Signal Sensor 1
3 | 0.75 RD/BU | 5291 | Ignition Voltage
4 | 0.5 BN/YE | 1664 | Heated Oxygen Sensor Low Signal Sensor 1

### Heated Oxygen Sensor (HO2S) 2

#### Connector Part Information

- OEM: ZMW4-7
- Service: Service by Harness - See Part Catalog
- Description: 4-Way M Sealed (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Heated Oxygen Sensor (HO2S) 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/BN | 1423 | Heated Oxygen Sensor Heater Low Control Sensor 2
2 | 0.5 BU | 1668 | Heated Oxygen Sensor High Signal Sensor 2
3 | 0.75 RD/BU | 5291 | Ignition Voltage
4 | 0.5 BN/YE | 1669 | Heated Oxygen Sensor Low Signal Sensor 2

### Heated Seat Element - Driver Cushion (KA1)

#### Connector Part Information

- OEM: 365058-2
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Junior Timer Series, (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Heated Seat Element - Driver Cushion (KA1)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1 WH | 2432 | Driver Heated Seat Cushion Element Supply Voltage
2 | 1 BN | 2150 | Ground
1 BN | 2150 | Ground

### Heated Seat Element - Passenger Cushion (KA1)

#### Connector Part Information

- OEM: 365058-2
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Junior Timer Series, (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Heated Seat Element - Passenger Cushion (KA1)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1 WH | 2436 | Passenger Heated Seat Cushion Element Supply Voltage
2 | 1 BN | 2150 | Ground
1 BN | 2150 | Ground

### Hood Ajar Switch

#### Connector Part Information

- OEM: 1452680-2
- Service: 93186673
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186673
- Release Tool/Test Probe: N/A

#### Hood Ajar Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/GN | 109 | Hood Ajar Switch Signal
2 | 0.5 BN | 1350 | Ground

### Horn

#### Connector Part Information

- OEM: ID406152
- Service: 21019425
- Description: 2-Way F GT 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 21019425
- Release Tool/Test Probe: N/A

#### Horn

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.5 BN/WH | 2026 | Low Note Horn Enable Signal
2 | 1.5 BN | 1050 | Ground

### HVAC Control Module, X1

#### Connector Part Information

- OEM: 967597-1
- Service: Service by Harness - See Part Catalog
- Description: 32-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### HVAC Control Module, X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | -- | Air Temperature Door Control A
2 | PU | -- | Mode Door Control A
3 | -- | -- | Not Used
4 | BN | -- | Recirculation Door Control A
5 | OG | 1542 | Battery Positive Voltage
6 | YE/GN | 839 | Run/Crank Ignition 1 Voltage
7 | BK | -- | Low Reference
8 | GY | -- | Air Temperature Actuator Sensor Signal
9 | YE | -- | Mode Actuator Sensor Signal
10 | -- | -- | Not Used
11 | BK/WH | 66 | A/C Request Signal
12 | BN/WH | 193 | Rear Defog Relay Control
13 | BU | 292 | Rear Defog Switch Signal
14-16 | -- | -- | Not Used
17 | RD | -- | Air Temperature Door Control B
18 | BU/RD | -- | Mode Door Control B
19 | -- | -- | Not Used
20 | OG/YE | -- | Recirculation Door Control B
21 | GN | 1382 | LED Dimming Signal
22 | BN/BK | -- | 8-Volt Reference
23 | YE/BK | 1650 | Ground
24-32 | -- | -- | Not Used

### HVAC Control Module, X2

#### Connector Part Information

- OEM:1534390-1
- Service: Service by Harness - See Part Catalog
- Description: 5-Way F Power Timer Series, (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### HVAC Control Module, X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN | -- | High Blower Motor Control
2 | BU | -- | Medium 2 Blower Motor Control
3 | PU | -- | Medium 1 Blower Motor Control
4 | OG | -- | Low Blower Motor Control
5 | RD | 1241 | Run Ignition 3 Voltage

### I/P Compartment - Lamp

#### Connector Part Information

- OEM: ID410224
- Service: 19178170
- Description: 2-Way F Flachsteckhülse 6,3 DIN46340 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 19178170
- Release Tool/Test Probe: N/A

#### I/P Compartment - Lamp

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 1650 | Ground
2 | 0.5 BK/YE | 1733 | Inadvertant Power Courtesy Lamp

### Ignition Control Module (ICM)

#### Connector Part Information

- OEM: ZFW 6-7
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Ignition Control Module (ICM)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 BN | 650 | Ground
2 | 1.5 BK | 39 | Run/Crank Ignition 1 Voltage
3 | 1 BU/YE | 2124 | Ignition Control 4
4 | 1 BU/GN | 2123 | Ignition Control 3
5 | 1 BU/WH | 2122 | Ignition Control 2
6 | 1 BU/RD | 2121 | Ignition Control 1

### Inflatable Restraints Front End Sensor - Left

#### Connector Part Information

- OEM: 1241905-4
- Service: 93181669
- Description: 2-Way F 64 MQS Series, Sealed (BK/BG)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93181669
- Release Tool/Test Probe: N/A

#### Inflatable Restraints Front End Sensor - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 6168 | Middle Front Impact Sensing Module Supply Voltage
2 | 0.5 OG/BK | 6169 | Middle Front Impact Sensing Module Signal

### Inflatable Restraint Front End Sensor - Right

#### Connector Part Information

- OEM: 5-1241905-5
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 64 MQS Series, Sealed (BG)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Front End Sensor - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE/GY | 6776 | Middle Front Impact Sensing Module 2 Supply Voltage
2 | 0.5 GN/WH | 6777 | Middle Front Impact Sensing Module 2 Signal

### Inflatable Restraint Front Passenger Presence System (PPS) Module

#### Connector Part Information

- OEM: 15332142
- Service: 89046638
- Description: 6-Way F GT 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 89046638
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Front Passenger Presence System (PPS) Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 BK | 1539 | Run/Crank Ignition 1 Voltage
B | 0.5 OG/WH | 5018 | Occupant Sensor Serial Data
C | 0.5 OG/VT | 353 | Passenger IP Module Suppression Indicator Control
D | 0.5 OG/BN | 2450 | Ground
E | 0.5 OG/BK | 371 | Passenger IP Module Disable Switch Signal
F | -- | -- | Not Used

### Inflatable Restraint I/P Module - X1

#### Connector Part Information

- OEM: 6 120 27 00
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (PU with OG Cover)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint I/P Module - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 OG/WH | 3024 | Passenger IP Module Stage 1 Low Control
2 | 0.5 WH | 3025 | Passenger IP Module Stage 1 High Control

### Inflatable Restraint I/P Module - X2

#### Connector Part Information

- OEM: 6 120 2700
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (YE with OG Cover)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint I/P Module - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 VT | 3026 | Passenger IP Module Stage 2 Low Control
2 | 0.5 OG/BK | 3027 | Passenger IP Module Stage 2 High Control

### Inflatable Restraint Steering Wheel Module - X1

#### Connector Part Information

- OEM: 6 120 27 00
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (PU with OG Cover)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Steering Wheel Module - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BU | 3020 | Steering Wheel Module Stage 1 Low Control
2 | WH | 3021 | Steering Wheel Module Stage 1 High Control

### Inflatable Restraint Steering Wheel Module - X2

#### Connector Part Information

- OEM: 6 120 27 00
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (YE with OG Cover)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Steering Wheel Module - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN | 3022 | Steering Wheel Module Stage 2 Low Control
2 | YE | 3023 | Steering Wheel Module Stage 2 High Control

### Inflatable Restraint Roof Rail Module - Left

#### Connector Part Information

- OEM: 12186799
- Service: 15306012
- Description: 2-Way M 280 Series (GN Encased in YE)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 15306012
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Roof Rail Module - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GN | 5020 | Left Front Head Curtain Module Low Control
2 | 0.5 OG/GN | 5019 | Left Front Head Curtain Module High Control

### Inflatable Restraint Roof Rail Module - Right

#### Connector Part Information

- OEM: 12186799
- Service: 15306012
- Description: 2-Way M 280 Series (GN Encased in YE)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly -15306012
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Roof Rail Module - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GY | 5022 | Right Front Head Curtain Module Low Control
2 | 0.5 OG/GY | 5021 | Right Front Head Curtain Module High Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM) - X1

#### Connector Part Information

- OEM: ZF56-10
- Service: Service by Harness - See Part Catalog
- Description: 56-Way F MX123 34576 Series (BN w/YE Lock)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-14 | -- | -- | Not Used
15 | 0.5 WH | 3025 | Passenger IP Module Stage 1 High Control
16 | 0.5 OG/WH | 3024 | Passenger IP Module Stage 1 Low Control
17 | 0.5 VT | 3026 | Passenger IP Module Stage 2 Low Control
18 | 0.5 OG/BK | 3027 | Passenger IP Module Stage 2 High Control
19-22 | -- | -- | Not Used
23 | 0.5 OG/BK | 3023 | Steering Wheel Module Stage 2 High Control
24 | 0.5 BK | 3022 | Steering Wheel Module Stage 2 Low Control
25 | 0.5 VT | 3020 | Steering Wheel Module Stage 1 Low Control
26 | 0.5 OG/VT | 3021 | Steering Wheel Module Stage 1 High Control
27-28 | -- | -- | Not Used
29 | 0.5 OG/WH | 5018 | Occupant Sensor Serial Data
30 | 0.5 OG/GY | 5246 | SIR Deployed Signal
31-33 | -- | -- | Not Used
34 | 0.5 BU/BK | 234 | Seat Belt Indicator Control
35 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
36 | -- | -- | Not Used
37 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
38 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
39-56 | -- | -- | Not Used

### Inflatable Restraint Sensing and Diagnostic Module (SDM) - X2

#### Connector Part Information

- OEM: ZF56-1 (2 Door) ZF56-2 (4 Door)
- Service: Service by Harness - See Part Catalog
- Description: 56-Way F MX123 34576 Series (GY w/YE Lock)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-15 | -- | -- | Not Used
16 | 0.75 OG/BN | 2450 | Ground
17 | 0.5 OG/GY | 5021 | Right Front Head Curtain Module High Control
18 | 0.5 GY | 5022 | Right Front Head Curtain Module Low Control
19 | 0.5 BU | 2117 | Passenger Seat Belt Pretensioner Low Control
20 | 0.5 OG/GY | 2116 | Passenger Seat Belt Pretensioner High Control
21 | 0.5 OG/GN | 5019 | Left Front Head Curtain Module High Control
22 | 0.5 GN | 5020 | Left Front Head Curtain Module Low Control
23 | 0.5 BK/WH | 2104 | Right Side Impact Module Low Control
24 | 0.5 OG/BK | 2103 | Right Side Impact Module High Control
25 | 0.5 OG/BN | 2118 | Driver Seat Belt Pretensioner High Control
26 | 0.5 BN | 2119 | Driver Seat Belt Pretensioner Low Control
27 | 0.5 BU | 2138 | Left Front Side Impact Module Low Control
28 | 0.5 OG/BU | 2137 | Left Front Side Impact Module High Control
29 | 0.75 BK | 3 | Run/Crank Ignition 1 Voltage
30 | 0.5 BK/WH | 6168 | Middle Front Impact Sensing Module Supply Voltage
31 | 0.5 OG/BK | 6169 | Middle Front Impact Sensing Module Signal
32 | 0.5 YE/GY | 6776 | Middle Front Impact Sensing Module 2 Supply Voltage
33 | 0.5 GN/WH | 6777 | Middle Front Impact Sensing Module 2 Signal
34 | 0.5 BN/WH | 238 | Driver Seat Belt Switch Signal
35 | 0.5 VT/BK | 1363 | Low Reference
36 | 0.5 BU | 1362 | Passenger Seat Belt Switch Signal
37 | 0.5 BU/BK | 1361 | Low Reference
38 | 0.5 BU/YE | 5056 | Passenger Seat Position Switch Signal
39 | 0.5 GN/WH | 2131 | Left Front Side Impact Sensing Module Supply Voltage
40 | 0.5 OG/GN | 2132 | Left Front Side Impact Sensing Module Signal
41 | 0.5 BN/WH | 2133 | Right Front Side Impact Sensing Module Supply Voltage
42 | 0.5 OG/BN | 2134 | Right Front Side Impact Sensing Module Signal
43-56 | -- | -- | Not Used

### Inflatable Restraint Side Impact Sensor (SIS) - Left

#### Connector Part Information

- OEM: 1241905-4
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 64 MQS Series, Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Side Impact Sensor (SIS) - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GN/WH | 2131 | Left Front Side Impact Sensing Module Supply Voltage
2 | 0.5 OG/GN | 2132 | Left Front Side Impact Sensing Module Signal

### Inflatable Restraint Side Impact Sensor (SIS) - Right

#### Connector Part Information

- OEM: 5-1241905-4
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 64 MQS Series, Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Side Impact Sensor (SIS) - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 2133 | Right Front Side Impact Sensing Module Supply Voltage
2 | 0.5 OG/BN | 2134 | Right Front Side Impact Sensing Module Signal

### Inflatable Restraint Steering Wheel Module Coil

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Steering Wheel Module Coil

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 YE | -- | --
4 | 0.5 GN | -- | --
5 | 0.5 BU | -- | --
6 | 0.5 PU | -- | --

### Inside Rearview Mirror (ISRVM)

#### Connector Part Information

- OEM: 917981-2
- Service: 15306351
- Description: 16-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Inside Rearview Mirror (ISRVM)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 OG/VT | 353 | Passenger IP Module Suppression Indicator Control
4 | 0.5 OG/BK | 371 | Passenger IP Module Disable Switch Signal
5-7 | -- | -- | Not Used
8 | 0.5 BN | 1550 | Ground
9-10 | -- | -- | Not Used
11 | 0.5 GN/WH | 2514 | Keypad Signal
12 | 0.5 OG/BK | 2518 | 10-Volt Reference
13 | 0.5 BK | 139 | Run/Crank Ignition 1 Voltage
14 | 0.5 YE/BK | 2516 | Keypad Green LED
15 | 0.5 BN/WH | 2517 | Keypad Red LED
16 | -- | -- | Not Used

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 1241727-1
- Service: 93186677
- Description: 42-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Instrument Panel Cluster (IPC)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-5 | -- | -- | Not Used
6 | 0.5 BK/WH | 292 | Rear Defog Switch Signal
7-9 | -- | -- | Not Used
10 | 0.5 BK/VT | 66 | A/C Request Signal (C60)
11 | 0.5 YE/RD | 1591 | Auto LED Control
12-13 | -- | -- | Not Used
14 | 0.5 BN/YE | 998 | MIL Control
15 | -- | -- | Not Used
16 | 0.75 RD | 1742 | Battery Positive Voltage
17 | 0.5 BK/VT | 1717 | Hazard Switch Indicator Control
18 | -- | -- | Not Used
19 | 0.5 GY/YE | 1382 | LED Dimming Signal
20 | 0.5 BN | 1650 | Ground
21 | 0.5 BN | 1650 | Ground
22-26 | -- | -- | Not Used
27 | 0.5 BK | 1039 | Run/Crank Ignition 1 Voltage
28 | 0.5 GY/BU | 192 | Front Fog Lamp Switch Signal (T96)
29 | 0.5 GY/VT | 44 | Instrument Panel Lamp Dimmer Switch Signal
30-32 | -- | -- | Not Used
33 | 0.5 YE | 1201 | Headlamp Low Beam
34 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
35 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
36 | 0.5 BN/YE | 1651 | Low Reference
37 | 0.5 GY/GN | 13 | Headlamp Switch Park Lamp Signal
38 | 0.5 BN/WH | 682 | Door Lock Lock/Unlock Signal
39 | 0.5 BK/BN | 1145 | Tire Inflation Monitor Reset Switch Signal
40 | 0.5 GN/WH | 111 | Hazard Switch Signal
41 | 0.5 YE/BK | 1436 | Auto Switch Signal
42 | 0.5 BN/WH | 193 | Rear Defog Relay Control

### Intake Manifold Tuning (IMT) Solenoid Valve

#### Connector Part Information

- OEM: 1-0967644-1
- Service: 93188697
- Description: 2-Way F 2.8 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93188697
- Release Tool/Test Probe: N/A

#### Intake Manifold Tuning (IMT) Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE/VT | 5041 | Intake Manifold Control 1
2 | 0.5 RD/BU | 5291 | Ignition Voltage

### Intake Manifold Tuning Valve (IMTV) Sensor

#### Connector Part Information

- OEM: ZFW 3-45
- Service: 19179748
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 19179748
- Release Tool/Test Probe: N/A

#### Intake Manifold Tuning Valve (IMTV) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 5042 | Intake Manifold Tuning Valve Sensor Signal
2 | 0.5 BN/YE | 5041 | Low Reference
3 | 0.5 BK/WH | 474 | 5 Volt Reference 1

### K50 Relay (C3U)

#### Connector Part Information

- OEM: 12034003
- Service: 88987189
- Description: 4-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88987189
- Release Tool/Test Probe: N/A

#### K50 Relay (C3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GN/WH | 129 | Sunroof Motor Close Control
2 | 0.75 BK | 1039 | Run/Crank Ignition 1 Voltage
3 | 0.75 BN | 1650 | Ground
4 | 0.5 BU/WH | 110 | Sunroof Switch Close Signal

### K93 Relay (MNF)

#### Connector Part Information

- OEM: 12034003
- Service: Service by Harness - See Part Catalog
- Description: 5-Way F Metri-Pack 630 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### K93 Relay (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BK | 539 | Run/Crank Ignition 1 Voltage
2 | 0.5 BN | 2150 | Ground
3 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal
4 | -- | -- | Not Used
5 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal

### Knock Sensor (KS)

#### Connector Part Information

- OEM: ZFW 2-30
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Knock Sensor (KS)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GY/BK | 496 | KS Signal
2 | 0.5 GY/RD | 1716 | KS Signal

### License Lamp - Left

#### Connector Part Information

- OEM: 1452680-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### License Lamp - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 2550 | Ground
2 | 0.5 GY/GN | 1255 | License Supply Voltage Signal

### License Lamp - Right

#### Connector Part Information

- OEM: 1452680-1
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### License Lamp - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 2550 | Ground
2 | 0.5 GY/GN | 1255 | License Supply Voltage Signal

### Liftgate Latch Assembly

#### Connector Part Information

- OEM: 15426710
- Service: Service by Harness - See Part Catalog
- Description: 4-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Liftgate Latch Assembly

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BN/WH | 5799 | Lift Gate Open/Close Motor Close Control
2 | 0.75 BN | 2550 | Ground
3 | 0.5 BK/BU | 1303 | Liftgate Ajar Switch Signal
4 | -- | -- | Not Used

### Liftgate Release Switch

#### Connector Part Information

- OEM: 968943-2
- Service: Service by Harness - See Part Catalog
- Description: 4-Way F 64 MQS Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Liftgate Release Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/YE | 5797 | Rear Closure Handle Switch Open Signal
2 | -- | -- | Not Used
3 | 0.5 BN | 2550 | Ground
4 | -- | -- | Not Used

### Mass Air Flow (MAF) / Intake Air Temperature (IAT) sensor

#### Connector Part Information

- OEM: 1.93E+09
- Service: Service by Harness - See Part Catalog
- Description: 4-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Mass Air Flow (MAF) / Intake Air Temperature (IAT) sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/VT | 469 | Low Reference
2 | 0.5 BN/GN | 472 | Intake Air Temperature Sensor Signal
3 | 0.5 GN/WH | 492 | Mass Air Flow Sensor Signal
4 | 0.5 RD/BU | 5291 | Ignition Voltage

### Mode Actuator

#### Connector Part Information

- OEM: 1-355082-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F MQS Series, (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Mode Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | -- | Low Reference
2 | YE | -- | Mode Actuator Sensor Signal
3 | BN/BK | -- | 8V Reference
4 | -- | -- | Not Used
5 | PU | -- | Mode Door Control A
6 | BU/RD | -- | Mode Door Control B

### Multifunction Switch - I/P

#### Connector Part Information

- OEM: 1355348-1
- Service: 93187174
- Description: 18-way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Multifunction Switch - I/P

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BN | 1650 | Ground
3 | 0.5 BN/GY | 1462 | Driver Heated Seat Switch Control
4 | 0.5 BK/BN | 1145 | Tire Inflation Monitor Reset Switch Signal
5 | 0.5 BN/WH | 682 | Door Lock Lock/Unlock Signal
6 | 0.5 GN/WH | 111 | Hazard Switch Signal
7 | -- | -- | Not Used
8 | 0.5 YE/BK | 1436 | Auto Switch Signal
9 | 0.5 BK/YE | 1505 | Front Passenger Heated Seat Switch Control
10 | -- | -- | Not Used
11 | 0.5 BU/BK | 234 | Seat Belt Indicator Control
12 | 0.5 BK | 1139 | Run/Crank Ignition 1 Voltage
13 | 0.5 BK | 1039 | Run/Crank Ignition 1 Voltage
14 | 0.5 VT/BN | 5968 | Driver Door Lock Status Indicator Signal
15 | 0.5 BK/VT | 1717 | Hazard Switch Indicator Control
16 | -- | -- | Not Used
17 | 0.5 YE/RD | 1591 | Auto LED Control
18 | 0.5 GY/YE | 1382 | LED Dimming Signal

### Neutral Control Solenoid Valve (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Neutral Control Solenoid Valve (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Low Reference
B | RD | 1527 | Shift Solenoid Supply Voltage 3

### Outside Rearview Mirror - Driver

#### Connector Part Information

- OEM: ID815839
- Service: Service by Harness - See Part Catalog
- Description: 18-Way F MQS Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Outside Rearview Mirror - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/WH | 6160 | Outside Left Mirror Vertical Position Control
2 | 0.5 GN/WH | 6159 | Outside Left Mirror Horizontal Position Control
3 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire
4-7 | -- | -- | Not Used
8 | 0.75 WH/BK | 2267 | Mirror Heating Element Supply Voltage
9 | 0.75 BN | 1550 | Ground
10-18 | -- | -- | Not Used

### Outside Rearview Mirror - Passenger

#### Connector Part Information

- OEM: ID815839
- Service: Service by Harness - See Part Catalog
- Description: 18-Way F MQS Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Outside Rearview Mirror - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/BK | 6162 | Outside Right Mirror Vertical Position Control
2 | 0.5 GN/BK | 6161 | Outside Right Mirror Horizontal Position Control
3 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire
4-7 | -- | -- | Not Used
8 | 0.75 WH/BK | 2267 | Mirror Heating Element Supply Voltage
9 | 0.75 BN | 1550 | Ground
10-18 | -- | -- | Not Used

### Park Brake Switch

#### Connector Part Information

- OEM: 13242.562.699
- Service: 93186705
- Description: 1-Way F 1.5 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186705
- Release Tool/Test Probe: N/A

#### Park Brake Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN/RD | 1134 | Park Brake Switch Signal

### Park/Neutral Position (PNP) Switch (MNF)

#### Connector Part Information

- OEM: ZFW10-2
- Service: Service by Harness - See Part Catalog
- Description: 10-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Park/Neutral Position (PNP) Switch (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 WH | 771 | Transmission Position Switch Bit 1 Signal
2 | 0.75 GN/WH | 772 | Transmission Position Switch Bit 2 Signal
3 | 0.75 GY | 773 | Transmission Position Switch Bit 3 Signal
4 | 0.75 WH/YE | 1371 | Transmission Position Switch Bit 4 Signal
5 | -- | -- | Not Used
6 | 2.5 BK/RD | 6 | Starter Solenoid Crank Voltage
7 | 0.75 BK/WH | 5007 | Reverse Switch Signal
8 | 0.75 BK | 539 | Run/Crank Ignition 1 Voltage
9 | 0.75 BN | 650 | Ground
10 | 2.5 BK/RD | 6 | Starter Solenoid Crank Voltage

### Position Lamp - Left

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Position Lamp - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | BK | 709 | Left Park Lamp Supply Voltage
-- | BK | 1150 | Ground

### Position Lamp - Right

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Position Lamp - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | BK | 309 | Right Park Lamp Supply Voltage
-- | BK | 1050 | Ground

### Power Steering Control Module (PSCM) - X1 (NS2/NR1)

#### Connector Part Information

- OEM: ZFW 3-45
- Service: Service by Harness - See Part Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Power Steering Control Module (PSCM) - X1 (NS2/NR1)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 639 | Run/Crank Ignition 1 Voltage
2 | 0.75 GN | 2500 | High Speed GMLAN Serial Data (+)
3 | 0.75 WH | 2501 | High Speed GMLAN Serial Data (-)

### Power Steering Control Module (PSCM) - X2

#### Connector Part Information

- OEM: ZFW 2-130
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Power Steering Control Module (PSCM) - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 10 RD | 702 | Battery Positive Voltage
2 | 10 BN | 150 | Ground

### Pressure Control (PC) Solenoid Valve (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Pressure Control (PC) Solenoid Valve (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GN | 5503 | Low Reference
B | OG | 1530 | Transmission Mainline Pressure Solenoid Control

### Radio - X1

#### Connector Part Information

- OEM: 30235101
- Service: 93186752
- Description: 40-Way F Mixed Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Radio - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 WH | 46 | Right Rear Speaker (+)
2 | 0.75 YE | 200 | Right Front Speaker (+)
3 | 0.75 BU | 201 | Left Front Speaker (+)
4 | 0.75 GN | 199 | Left Rear Speaker (+)
5 | 0.75 BN/WH | 115 | Right Rear Speaker Signal (-)
6 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-)
7 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-)
8 | 0.75 BN/GN | 116 | Left Rear Speaker Signal (-)
9 | 0.5 GN | 5169 | Mid Speed GMLAN Serial Data (+)
10 | 0.5 WH | 5170 | Mid Speed GMLAN Serial Data (-)
11 | 0.5 BK | 693 | Cellular Telephone Mute Signal
12 | 2.5 BN | 1750 | Ground
13 | -- | -- | Not Used
14 | 0.5 WH/BN | 1960 | Front Center Speaker (-)
15 | 2.5 RD | 3040 | Battery Positive Voltage
16 | 0.5 YE/WH | 1860 | Front Center Speaker (+)
17-30 | -- | -- | Not Used
31 | 0.35 VT/WH | 5839 | Left Auxiliary Audio Signal 2
32 | 0.35 VT/RD | 5841 | Right Auxiliary Audio Signal 2
33 | -- | -- | Not Used
34 | 0.5 YE | 658 | Cellular Telephone Voice Signal
35-37 | -- | -- | Not Used
38 | 0.35 BK | 5842 | Auxiliary Audio Screen 2
39 | -- | -- | Not Used
40 | 0.5 YE/BN | 659 | Low Reference

### Rear Window Defogger Grid - X1

#### Connector Part Information

- OEM: 16000.649.696
- Service: Service by Harness - See Part Catalog
- Description: 1-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Rear Window Defogger Grid - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 BK | 293 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid - X2

#### Connector Part Information

- OEM: 16000.649.696
- Service: Service by Harness - See Part Catalog
- Description: 1-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Rear Window Defogger Grid - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 BN | 2550 | Ground

### Rear Window Wiper Motor

#### Connector Part Information

- OEM: ID601807
- Service: Service by Harness - See Part Catalog
- Description: 3-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Rear Window Wiper Motor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 1.5 BU | 393 | Rear Window Wiper Motor Control
B | 1.5 BN | 2550 | Ground
C | 1.5 BK | 1939 | Run/Crank Ignition 1 Voltage

### Recirculation Actuator

#### Connector Part Information

- OEM:12047662
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Metri-Pack 150 Series, (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Recirculation Actuator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | -- | Recirculation Door Control A
B | OG/YE | -- | Recirculation Door Control B

### Repeater Lamp - Left Front

#### Connector Part Information

- OEM: E0146
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Bulb Base (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Repeater Lamp - Left Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 GY/BK | 2114 | Left Turn Signal Lamp Supply Voltage
B | 0.5 BN | 1150 | Ground

### Repeater Lamp - Right Front

#### Connector Part Information

- OEM: E0146
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Bulb Base (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Repeater Lamp - Right Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 GY/GN | 2115 | Right Turn Signal Lamp Supply Voltage
B | 0.5 BN | 1050 | Ground

### Seat Position Sensor - Passenger

#### Connector Part Information

- OEM: 89047381
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Seat Position Sensor - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 1361 | Low Reference
2 | 0.35 BK | 5056 | Passenger Seat Position Switch Signal

### Side Marker Lamp - Left Front

#### Connector Part Information

- OEM: E-5229
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Side Marker Lamp - Left Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 1414 | Left Front Turn Signal Switch Signal
2 | 0.5 BN | 1150 | Ground

### Side Marker Lamp - Left Rear

#### Connector Part Information

- OEM: E-5229
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Side Marker Lamp - Left Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 2550 | Ground
2 | 0.5 GY/GN | 1255 | Side Marker/License Supply Voltage Signal

### Side Marker Lamp - Right Front

#### Connector Part Information

- OEM: E-5229
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Side Marker Lamp - Right Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/GN | 1415 | Right Front Turn Signal Switch Signal
2 | 0.5 BN | 1050 | Ground

### Side Marker Lamp - Right Rear

#### Connector Part Information

- OEM: E-5229
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Side Marker Lamp - Right Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 2550 | Ground
2 | 0.5 GY/GN | 1255 | Side Marker/License Supply Voltage Signal

### Speaker - Center I/P

#### Connector Part Information

- OEM: 968943-3
- Service: 93184057
- Description: 4-Way F 64 MQS Series (BN)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93184057
- Release Tool/Test Probe: N/A

#### Speaker - Center I/P

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE/WH | 1860 | Front Center Speaker (+)
2-3 | -- | -- | Not Used
4 | 0.5 WH/BN | 1960 | Front Center Speaker (-)

### Speaker - Left Front Tweeter (U65)

#### Connector Part Information

- OEM: ID404665
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F FASTIN-FASTON 2.8 Series (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Speaker - Left Front Tweeter (U65)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-)
2 | 0.75 BU | 201 | Left Front Speaker (+)

### Speaker - Left Front

#### Connector Part Information

- OEM: ID404665
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F FASTIN-FASTON 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Speaker - Left Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BU | 201 | Left Front Speaker (+)
2 | 0.75 BN/BU | 118 | Left Front Speaker Signal (-)

### Speaker - Left Rear

#### Connector Part Information

- OEM: ID404665
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F FASTIN-FASTON 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Speaker - Left Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 GN | 199 | Left Rear Speaker (+)
2 | 0.75 BN/GN | 116 | Left Rear Speaker Signal (-)

### Speaker - Right Front

#### Connector Part Information

- OEM: ID404665
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F FASTIN-FASTON 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Speaker - Right Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 YE | 200 | Right Front Speaker (+)
2 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-)

### Speaker - Right Front Tweeter (U65)

#### Connector Part Information

- OEM: ID404665
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F FASTIN-FASTON 2.8 Series (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Speaker - Right Front Tweeter (U65)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 BN/YE | 117 | Right Front Speaker Signal (-)
2 | 0.75 YE | 200 | Right Front Speaker (+)

### Speaker - Right Rear

#### Connector Part Information

- OEM: ID404665
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F FASTIN-FASTON 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Speaker - Right Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 WH | 46 | Right Rear Speaker (+) (3 Door)
0.75 GN | 199 | Right Rear Speaker (+) (5 Door)
2 | 0.75 BN/WH | 115 | Right Rear Speaker Signal (-) (3 Door)
0.75 BN/GN | 116 | Right Rear Speaker Signal (-) (5 Door)

### Starter - X1

#### Connector Part Information

- Terminal: S4.3-8
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Starter - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | 25 RD | 1B | Battery Positive Voltage
-- | 16 RD | 1 | Battery Positive Voltage

### Starter - X2

#### Connector Part Information

- Terminal: S4.3-8
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Starter - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
-- | 2.5 BK/RD | 6 | Starter Solenoid Crank Voltage

### Steering Wheel Control Switch - Left

#### Connector Part Information

- OEM:See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 4-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Steering Wheel Control Switch - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN | -- | --
2 | PU | -- | --
3 | RD | -- | --
4 | GY | -- | --

### Steering Wheel Control Switch - Right

#### Connector Part Information

- OEM:See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Steering Wheel Control Switch - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | -- | Low Reference
2 | BN | -- | Horn Switch Signal
3 | RD | -- | --
4 | YE | -- | --
5 | GY | -- | --
6 | BU | -- | --

### Steering Column Control Module

#### Connector Part Information

- OEM: 1241726-1
- Service: Service by Harness - See Part Catalog
- Description: 32-Way F (YE Encased in BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Steering Column Control Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.75 RD | 1540 | Battery Positive Voltage
2 | 0.75 BK | 3 | Run/Crank Ignition 1 Voltage
3 | -- | -- | Not Used
4 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
5 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
6 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
7 | 0.75 BN | 1650 | Ground
8-10 | -- | -- | Not Used
11 | 0.5 VT | 3020 | Steering Wheel Module Stage 1 Low Control
12 | 0.5 OG/VT | 3021 | Steering Wheel Module Stage 1 High Control
13 | -- | -- | Not Used
14 | 0.5 BK | 3022 | Steering Wheel Module Stage 2 Low Control
15 | 0.5 OG/BK | 3023 | Steering Wheel Module Stage 2 High Control
16 | -- | -- | Not Used
17 | 0.5 BN/GN | 1884 | Ignition Voltage
18 | -- | -- | Not Used
19 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
20 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
21 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
22 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
23-32 | -- | -- | Not Used

### Stop Lamp Switch

#### Connector Part Information

- OEM: 968943-2
- Service: 93186707
- Description: 4-Way F 64 MQS Series (GY)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186707
- Release Tool/Test Probe: N/A

#### Stop Lamp Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 RD | 302 | Battery Positive Voltage
2 | 0.5 BN/GY | 17 | Stop Lamp Switch Signal
3 | 0.5 RD/BU | 5293 | Ignition Voltage
4 | 0.5 BK/BN | 848 | Brake Switch Signal

### Sunroof Control Module (C3U)

#### Connector Part Information

- OEM: 927458-1
- Service: Service by Harness - See Part Catalog
- Description: 12-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Sunroof Control Module (C3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 OG | 110 | Sunroof Switch Close Signal
2 | 0.5 BN | -- | Sunroof Motor Close Control
3 | 0.5 PK | -- | Sunroof Open/Closed Signal
4 | 0.5 BU | 4 | Accessory Voltage
5 | 2.5 RD | 140 | Battery Positive Voltage
6 | 2.5 BK | 1550 | Ground
7 | 0.5 GY | -- | Not Used
8-12 | -- | -- | Not Used

### Sunroof Shade Module (C3U)

#### Connector Part Information

- OEM: 927458-1
- Service: Service by Harness - See Part Catalog
- Description: 12-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Sunroof Shade Module (C3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 OG | -- | Sunroof Shade Switch Close Signal
2 | 0.5 BN | -- | Sunroof Shade Switch Open Signal
3 | 0.5 PK | -- | Sunroof Open/Closed Signal
4 | -- | -- | Not Used
5 | 2.5 RD | 142 | Battery Positive Voltage
6 | 2.5 BK | 1550 | Ground
7-12 | -- | -- | Not Used

### Sunroof Shade Switch (C3U)

#### Connector Part Information

- OEM: 968291-2
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Micro Quadlok Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Sunroof Shade Switch (C3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 OG | -- | Sunroof Shade Switch Close Signal
3 | 0.5 RD | 1382 | LED Dimming Signal
4 | 0.5 BK | 1550 | Ground
5 | 0.5 BN | -- | Sunroof Shade Switch Open Signal
6 | 0.5 BK | 1550 | Ground

### Sunroof Switch (C3U)

#### Connector Part Information

- OEM: 2-968291-1
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Micro Quadlok Series (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Sunroof Switch (C3U)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 OG | 129 | Sunroof Motor Close Control
3 | 0.5 RD | 1382 | LED Dimming Signal
4 | 0.5 BK | 1550 | Ground
5 | 0.5 BN | -- | Sunroof Motor Close Control
6 | 0.5 BK | 1550 | Ground

### Sunshade - Left

#### Connector Part Information

- OEM: ID401561
- Service: 93182537
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93182537
- Release Tool/Test Probe: N/A

#### Sunshade - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 RD/BU | 1732 | Inadvertant Power Courtesy Lamp
B | 0.5 BN | 1550 | Ground

### Sunshade - Right

#### Connector Part Information

- OEM: ID401561
- Service: 93182537
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93182537
- Release Tool/Test Probe: N/A

#### Sunshade - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 RD/BU | 1732 | Inadvertant Power Courtesy Lamp
B | 0.5 BN | 1550 | Ground

### Tail Lamp - Left

#### Connector Part Information

- OEM: ID404398
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Tail Lamp - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1.5 BN | 2550 | Ground (3 Door)
0.5 WH/BK | 5219 | Left Backup Lamp Supply Voltage (5 Door)
2 | 0.5 WH/BK | 5219 | Left Backup Lamp Supply Voltage (3 Door)
3 | -- | -- | Not Used
4 | 0.5 BK/YE | 5221 | Left Brake Lamp Supply Voltage (5 Door)
5 | 0.5 BK/WH | 1334 | Left Rear Turn Signal Lamp Supply Voltage
6 | 0.5 BK/YE | 5221 | Left Brake Lamp Supply Voltage (3 Door)
1.5 BN | 2550 | Ground (5 Door)

### Tail Lamp - Right

#### Connector Part Information

- OEM: ID404398
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Tail Lamp - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK/YE | 5222 | Right Brake Lamp Supply Voltage (3 Door)
1.5 BN | 2550 | Ground (5 Door)
2 | 0.5 BK/GN | 1335 | Right Rear Turn Signal Lamp Supply Voltage
3 | 0.5 BK/YE | 5222 | Right Brake Lamp Supply Voltage (5 Door)
4 | -- | -- | Not Used
5 | 0.5 WH/BK | 5220 | Right Backup Lamp Supply Voltage (3 Door)
6 | 1.5 BN | 2550 | Ground (3 Door)
0.5 WH/BK | 5220 | Right Backup Lamp Supply Voltage (5 Door)

### Throttle Body

#### Connector Part Information

- OEM: FEP 42121700
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Throttle Actuator Control (TAC) Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 485 | Throttle Position Sensor Signal 1
2 | 0.5 BK/WH | 2701 | 5 Volt Reference 2
3 | 1 BK/WH | 581 | Throttle Actuator Control Open
4 | 0.5 BU | 486 | Throttle Position Sensor Signal 2
5 | 1 BN/WH | 582 | Throttle Actuator Control Close
6 | 0.5 BN/WH | 2752 | Low Reference

### Tire Pressure Module

#### Connector Part Information

- OEM: 968473-1
- Service: 93187175
- Description: 12-Way F 64 MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Tire Pressure Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 GN | 5060 | Low Speed GMLAN Serial Data
2 | -- | -- | Not Used
3 | 0.5 BK | 239 | Run/Crank Ignition 1 Voltage
4 | 0.5 BN | 1650 | Ground
5-12 | -- | -- | Not Used

### Torque Converter Clutch (TCC) Solenoid Valve (MNF)

#### Connector Part Information

- OEM: See Catalog
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Torque Converter Clutch (TCC) Solenoid Valve (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN | 2879 | Low Reference
B | YE | 1994 | TCC PWM Solenoid Valve Control

### Transmission Control Module (TCM) (MNF)

#### Connector Part Information

- OEM: 1241727-1
- Service: Service by Harness - See Part Catalog
- Description: 42-Way F MQS Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Transmission Control Module (TCM) (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE/RD | 1230 | Transmission Speed Sensor Signal
2 | 0.5 YE/BN | 401 | Low Reference
3 | 0.5 GN | 772 | Transmission Position Switch Bit 2 Signal
4 | 0.5 WH | 771 | Transmission Position Switch Bit 1 Signal
5 | 0.5 GN | 1078 | Ignition Key/Shifter Interlock Solenoid Lock Signal
6-9 | -- | -- | Not Used
10 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
11 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
12-13 | -- | -- | Not Used
14 | 0.5 BU/WH | 5503 | Low Reference
15 | 0.5 BN/GN | 2879 | Low Reference
16 | 0.5 WH/GN | 1530 | Transmission Mainline Pressure Solenoid Control
17 | 0.5 WH/BK | 1994 | TCC PWM Solenoid Valve Control
18 | 0.5 BK/WH | 1527 | Shift Solenoid Supply Voltage 3
19 | 0.5 BK/VT | 1526 | Shift Solenoid Supply Voltage 2
20 | 0.5 BK/GN | 1525 | Shift Solenoid Supply Voltage 1
21 | 0.75 BK | 539 | Run/Crank Ignition 1 Voltage
22 | 0.5 YE/BK | 1231 | Low Reference
23 | 0.5 YE/VT | 400 | Vehicle Speed Sensor Signal
24 | 0.5 WH/YE | 1371 | Transmission Position Switch Bit 4 Signal
25 | 0.5 GY | 773 | Transmission Position Switch Bit 3 Signal
26-30 | -- | -- | Not Used
31 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
32 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
33-34 | -- | -- | Not Used
35 | 0.5 BU/YE | 488 | Winter Mode Switch Signal
36 | -- | -- | Not Used
37 | 0.5 BK/BU | 585 | Transmission Oil Temperature Sensor Signal
38 | 0.5 BN/BK | 586 | Low Reference
39 | 0.5 BN | 2150 | Ground
40 | 0.5 BN | 2150 | Ground
41 | 0.75 RD | 3740 | Battery Positive Voltage
42 | 0.75 BK | 539 | Run/Crank Ignition 1 Voltage

### Vehicle Communication Interface Module (VCIM) Battery

#### Connector Part Information

- OEM: ID401561
- Service: 93182537
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93182537
- Release Tool/Test Probe: N/A

#### Vehicle Communication Interface Module (VCIM) Battery

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 5235 | Battery Backup Supply Voltage
B | 0.5 GY/BK | 5167 | Low Reference

### Vehicle Communications Interface Module (VCIM) - Left - X1

#### Connector Part Information

- OEM: 917981-1
- Service: 15306351
- Description: 16-Way F (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Vehicle Communications Interface Module (VCIM) - Left - X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BN/WH | 2517 | Keypad Red LED
3 | 0.5 YE/BK | 2516 | Keypad Green LED
4-5 | -- | -- | Not Used
6 | 0.5 OG/BK | 2518 | 10-Volt Reference
7 | -- | -- | Not Used
8 | 0.75 BN | 1750 | Ground
9-10 | -- | -- | Not Used
11 | 0.5 GN/WH | 2514 | Keypad Signal
12 | -- | -- | Not Used
13 | 0.5 GY/BK | 5167 | Low Reference
14 | 0.5 RD/WH | 5235 | Battery Backup Supply Voltage
15 | 0.75 RD | 3140 | Battery Positive Voltage
16 | -- | -- | Not Used

### Vehicle Communications Interface Module (VCIM) - Left - X2

#### Connector Part Information

- OEM: 917975-1
- Service: 88952886
- Description: 12-Way F (WH)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Vehicle Communications Interface Module (VCIM) - Left - X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE | 658 | Cellular Telephone Voice Signal
2 | 0.5 YE/BN | 659 | Low Reference
3-4 | -- | -- | Not Used
5 | 0.5 BN/VT | 1132 | DLC Class 2 Serial Data
6 | 0.5 YE | 710 | Class 2 Serial Data Secondary
7 | -- | -- | Not Used
8 | 0.5 BK | 5842 | Auxiliary Audio Screen 2
9 | 0.35 BU/RD | 5191 | Cellular Telephone Microphone Signal
10 | 0.35 BK | 5193 | Low Reference
11 | -- | -- | Not Used
12 | 0.5 BK | 693 | Cellular Telephone Mute Signal

### Vehicle Communications Interface Module (VCIM) - Left - X4

#### Connector Part Information

- OEM: 638695-2
- Service: 88988545
- Description: 12-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Vehicle Communications Interface Module (VCIM) - Left - X4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
3 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
4-7 | -- | -- | Not Used
8 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
9 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
10-12 | -- | -- | Not Used

### Vehicle Communications Interface Module (VCIM) - Left - X5

#### Connector Part Information

- OEM: T00100B1300
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M (Metal)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Vehicle Communications Interface Module (VCIM) - Left - X5

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.35 BK | 6797 | GSM Antenna Screen
2 | 0.35 BK | 6794 | GSM Antenna Signal

### Vehicle Communications Interface Module (VCIM) - Left - X6

#### Connector Part Information

- OEM: 59K28A-102A4-Y
- Service: Service by Harness - See Part Catalog
- Description: 2-Way M (BU)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Vehicle Communications Interface Module (VCIM) - Left - X6

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.35 BK | 5175 | Antenna Navigation Screen
2 | 0.35 BK | 5174 | Antenna Navigation Signal

### Vehicle Communications Interface Module (VCIM) - Right

#### Connector Part Information

- OEM: 175966-2
- Service: 88975902
- Description: 16-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Vehicle Communications Interface Module (VCIM) - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 YE | 710 | Class 2 Serial Data Secondary
2 | -- | -- | Not Used
3 | 0.5 WH | 194 | Door Unlock Control
4 | 0.5 BN/WH | 28 | Horn Relay Control
5-8 | -- | -- | Not Used
9 | 0.5 BU/BN | 1903 | ABS Wheel Speed Sensor Signal Left Front
10 | 0.5 OG/GY | 5246 | SIR Deployed Signal
11 | -- | -- | Not Used
12 | 0.5 BN/GN | 1884 | Ignition Voltage
13 | 0.5 BK | 3 | Run/Crank Ignition 1 Voltage
14 | 0.5 RD | 3140 | Battery Positive Voltage
15 | 0.5 BN | 1750 | Ground
16 | -- | -- | Not Used

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

- OEM: 2880 4147 0773
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Wheel Speed Sensor (WSS) - Left Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/WH | 830 | Wheel Speed Sensor Signal Left Front
2 | 0.5 BN/WH | 873 | Low Reference

### Wheel Speed Sensor (WSS) - Left Rear

#### Connector Part Information

- OEM: 15397337
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Wheel Speed Sensor (WSS) - Left Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU | 884 | Wheel Speed Sensor Signal Left Rear
2 | 0.5 BN/BU | 885 | Low Reference

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

- OEM: 2880 4147 0773
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Wheel Speed Sensor (WSS) - Right Front

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/RD | 872 | Wheel Speed Sensor Signal Right Front
2 | 0.5 BN/RD | 833 | Low Reference

### Wheel Speed Sensor (WSS) - Right Rear

#### Connector Part Information

- OEM: 15397337
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Wheel Speed Sensor (WSS) - Right Rear

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BU/RD | 882 | Wheel Speed Sensor Signal Right Rear
2 | 0.5 BN/RD | 883 | Low Reference

### Window Motor - Driver

#### Connector Part Information

- OEM: ID404743
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Motor - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 RD | 2040 | Battery Positive Voltage
2 | 0.5 WH/GN | 1300 | Power Window Master Switch Left Front Up Signal
3 | 0.5 GY | 1136 | Power Window Master Switch Left Front Down Signal
4 | 2.5 BN | 1550 | Ground
5 | -- | -- | Not Used
6 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal

### Window Motor - Left Rear (5 Door)

#### Connector Part Information

- OEM: ID404743
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Motor - Left Rear (5 Door)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 RD | 2240 | Battery Positive Voltage
2 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal
3 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal
4 | 2.5 BN | 2350 | Ground
5 | -- | -- | Not Used
6 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal

### Window Motor - Passenger

#### Connector Part Information

- OEM: ID404743
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Motor - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 RD | 2140 | Battery Positive Voltage
2 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal
3 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal
4 | 2.5 BN | 1550 | Ground
5 | -- | -- | Not Used
6 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal

### Window Motor - Right Rear (5 Door)

#### Connector Part Information

- OEM: ID404743
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Motor - Right Rear (5 Door)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 RD | 2240 | Battery Positive Voltage
2 | 0.5 VT/GN | 168 | Power Window Master Switch Right Rear Up Signal
3 | 0.5 VT/BN | 169 | Power Window Master Switch Right Rear Down Signal
4 | 2.5 BN | 2350 | Ground
5 | -- | -- | Not Used
6 | 0.5 BN/BK | 5200 | Power Window Comfort Close Signal

### Window Switch - Driver

#### Connector Part Information

- OEM: 968265-1
- Service: Service by Harness - See Part Catalog
- Description: 32-Way F 0.64 Quadlock Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Switch - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-7 | -- | -- | Not Used
8 | 0.5 BU/BN | 171 | Power Window Master Switch Right Rear Down Signal (5 Door)
9 | 0.5 BU/GN | 170 | Power Window Master Switch Right Rear Up Signal (5 Door)
10 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal (5 Door)
11 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal
12 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal
13 | -- | -- | Not Used
14 | 0.5 BU/BK | 6162 | Outside Right Mirror Vertical Position Control
15 | 0.5 GN/BK | 6161 | Outside Right Mirror Horizontal Position Control
16-23 | -- | -- | Not Used
24 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal (5 Door)
25 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal (5 Door)
26 | 0.5 BK | 4 | Accessory Voltage
27 | 0.5 GY | 1136 | Power Window Master Switch Left Front Down Signal
28 | 0.5 WH/GN | 1300 | Power Window Master Switch Left Front Up Signal
29 | 0.5 BN | 6163 | Outside Mirror Position Motor Drain Wire
30 | 0.5 BU/WH | 6160 | Outside Left Mirror Vertical Position Control
31 | 0.5 GN/WH | 6159 | Outside Left Mirror Horizontal Position Control
32 | 0.75 BN | 1550 | Ground

### Window Switch - Left Rear (5 Door)

#### Connector Part Information

- OEM: 1-0968291-2
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Micro Quadlok Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Switch - Left Rear (5 Door)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal
2 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal
3 | 0.5 VT/BN | 169 | Power Window Master Switch Left Rear Down Signal
4 | 0.5 BN | 2350 | Ground
5 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal
6 | 0.5 VT/GN | 168 | Power Window Master Switch Left Rear Up Signal

### Window Switch - Passenger

#### Connector Part Information

- OEM: 1-0968291-2
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Micro Quadlok Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Switch - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 4 | Accessory Voltage
2 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal
3 | 0.5 YE/BN | 167 | Power Window Master Switch Right Front Down Signal
4 | 0.5 BN | 2050 | Ground
5 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal
6 | 0.5 YE/GN | 166 | Power Window Master Switch Right Front Up Signal

### Window Switch - Right Rear (5 Door)

#### Connector Part Information

- OEM: 1-0968291-2
- Service: Service by Harness - See Part Catalog
- Description: 6-Way F Micro Quadlok Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Window Switch - Right Rear (5 Door)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 WH/BU | 1307 | Power Window Master Switch Lockout Signal
2 | 0.5 VT/BN | 169 | Power Window Master Switch Right Rear Down Signal
3 | 0.5 VT/BN | 169 | Power Window Master Switch Right Rear Down Signal
4 | 0.5 BN | 2350 | Ground
5 | 0.5 VT/GN | 168 | Power Window Master Switch Right Rear Up Signal
6 | 0.5 VT/GN | 168 | Power Window Master Switch Right Rear Up Signal

### Windshield Outside Moisture Sensor

#### Connector Part Information

- OEM: 968705-1
- Service: 88953152
- Description: 3-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88953152
- Release Tool/Test Probe: N/A

#### Windshield Outside Moisture Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BK | 139 | Run/Crank Ignition 1 Voltage
2 | 0.5 BK | 1550 | Ground
3 | 0.5 GN | 481 | Rain Sense Signal 1

### Windshield Washer Fluid Level Switch

#### Connector Part Information

- OEM: 1452680-1
- Service: 93186680
- Description: 2-Way F 1.2 Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186680
- Release Tool/Test Probe: N/A

#### Windshield Washer Fluid Level Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 BN | 1150 | Ground
2 | 0.5 GN/WH | 99 | Windshield Washer Fluid Level Sensor Signal

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: ID401589
- Service: 93186714
- Description: 2-Way F Mini Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93186714
- Release Tool/Test Probe: N/A

#### Windshield Washer Fluid Pump

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 1 BK/RD | 228 | Windshield Washer Pump Control
2 | 1 BK/VT | 392 | Rear Window Washer Pump Control

### Windshield Wiper Motor

#### Connector Part Information

- OEM: 42122100
- Service: 93191103
- Description: 4-Way F 2. 8 Junior Power Timer Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 93191103
- Release Tool/Test Probe: N/A

#### Windshield Wiper Motor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 2.5 WH | 92 | Windshield Wiper Motor High Speed Control
2 | 2.5 YE | 95 | Windshield Wiper Motor Low Speed Control
3 | 0.5 BN/GN | 196 | Windshield Wiper Motor Park Switch Signal
4 | 2.5 BN | 1350 | Ground

### Winter Mode Switch (MNF)

#### Connector Part Information

- OEM: ID608416
- Service: Service by Harness - See Part Catalog
- Description: 4-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: Service by Harness - See Part Catalog
- Release Tool/Test Probe: N/A

#### Winter Mode Switch (MNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.5 BU/YE | 488 | Winter Mode Switch Signal
B | 0.5 BN | 2150 | Ground
C | -- | -- | Not Used
D | 0.75 BK | 539 | Run/Crank Ignition 1 Voltage

### Yaw and Lateral Accelerometer Sensor (FX3)

#### Connector Part Information

- OEM: 2-967616-1
- Service: 88953345
- Description: 6-Way F MQS Socket Housing, Sealed (GY with BK Housing)

#### Terminal Part Information

- Terminal/Tray: Service by Connector Assembly - 88953345
- Release Tool/Test Probe: N/A

#### Yaw and Lateral Accelerometer Sensor (FX3)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | 0.5 WH | 2501 | High Speed GMLAN Serial Data (-)
2 | 0.5 GN | 2500 | High Speed GMLAN Serial Data (+)
3 | 0.5 GN/BK | 1338 | Yaw Rate Sensor Signal 2
4 | -- | -- | Not Used
5 | 0.5 GY/BK | 1337 | Yaw Rate Sensor Volt Reference
6 | -- | -- | Not Used