For 1990-2009 cars

### Removal Procedure

1. Remove the vertical adjustment for front seat. Refer to Front Seat Vertical Adjuster Replacement .
2. Remove the seat spring mat.

• | Unhook the seat spring mat (1) (arrows).

• | Remove the seat spring mat.

### Installation Procedure

1. Install the seat spring mat.

Insert the seat spring mat.

2. Install the vertical adjustment for front seat. Refer to Front Seat Vertical Adjuster Replacement .