For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Holder Bolt | 7 N·m | 62 lb in
Battery Shield Bolt | 10 N·m | 89 lb in
Battery Support Bolts | 15 N·m | 11 lb ft
Brake Fluid Reservoir to Brake Master Cylinder Bolt | 6 N·m | 53 lb in
Brake Hose to Brake Caliper Banjo Bolt | 40 N·m | 30 lb ft
Brake Line to Brake Hose Clamping Plate | 14 N·m | 124 lb in
Brake Line to Brake Master Cylinder Retaining Bolts | 14 N·m | 124 lb in
Brake Line to Hydraulic Modulator and Brake Master Cylinder | 14 N·m | 124 lb in
Brake Master Cylinder Nuts | 21 N·m | 16 lb ft
Brake Master Cylinder to Brake Servo Nuts | 21 N·m | 16 lb ft
Brake Pedal with Bearing Block Bolts and Nuts | 20 N·m | 15 lb ft
Brake Servo to Bulkhead Nuts | 20 N·m | 15 lb ft
Footwell Paneling Bolts - Driver Side | 2.5 N·m | 22 lb in
Hydraulic Line Retaining Bolts | 14 N·m | 124 lb in
Hydraulic Modulator Bolts | 8 N·m | 71 lb in
Hydraulic Modulator Bracket Bolts | 20 N·m | 15 lb ft
Instrument Panel Padding Bolts - Lower | 2.5 N·m | 22 lb in
Intermediate Spindle to Steering Gear Bolts | 24 N·m | 18 lb ft
Spindle to Steering Spindle Bolt | 24 N·m | 18 lb ft
Steering Column Support Tube Bottom Bolts | 0.7 N·m | 6.2 lb in
Steering Column Support Tube Top Bolts | 0.7 N·m | 6.2 lb in
Vacuum Hose Connections | 24 N·m | 18 lb ft
Wheel Bolts - Front | 110 N·m | 81 lb ft