For 1990-2009 cars

### Removal Procedure

1. Remove the central console of the storage compartment, rear.

1.1. | Remove the upwards.

1.2. | Remove the 8 clips.

2. Remove the ashtray insert.

2.1. | Loosen the fastening clamp.

2.2. | Remove the ashtray insert .

3. Remove the ashtray.

3.1. | Remove the 2 clips (1).

3.2. | Remove the ashtray.

### Installation Procedure

1. Install the ashtray.

Insert the 2 clips.

2. Install the ashtray insert.
3. Install the rear central console storage compartment.

Insert the 8 clips.