For 1990-2009 cars

### Removal Procedure

Important: Drain the washer solvent into a suitable container.

Remove the pump for the headlamp washer system (1).

• | Disconnect the hose (3).

• | Remove the washer pump upward.

• | Disconnect the wiring harness plug (2).

### Installation Procedure

1. Install the pump for the headlamp washer system.

• | Connect the wiring harness plug.

• | Insert the washer pump.

• | Connect the hose.

2. Top up the washer fluid.