For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Warning in the Preface section.

Note: When replacing the control unit, before removing, carry out a Reset using the Tech 2. Refer to Control Module References.

1. Disconnect the battery.
2. Remove the steering wheel. Refer to Steering Wheel Replacement.
3. Remove the lower steering column paneling.

• | Remove the 5 bolts (arrows).

• | Remove the ignition lock panel (1).

• | Remove the rubber sleeve out of the steering column paneling.

4. Remove the column integration module (CIM).

• | Remove the 3 bolts (1).

• | Remove the wiring harness holder (arrow).

• | Release the wiring harness plug (2) and disconnect.

Note: Disconnect the engaging lug with a suitable tool (1), a hex screwdriver 1.5 mm WAF.

5. Remove the turn signal multifunction switch.

• | Remove the retaining lug.

• | Remove the actuating lever.

Note:

• | The CIM replaces the existing contact unit and contains additional functions.

• | The contact unit may not be twisted when it has been removed.

• | When removing and installing, ensure that the markings (arrows) are opposite each other as shown in the illustration.

6. Remove the CIM.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the CIM.

• | Connect and lock the wiring harness plug.

• | Install the wiring harness holder.

Tighten
Tighten the 3 bolts to 3.5 N·m (32 lb in).

2. Install the actuating lever.

• | Engage the actuating lever.

• | Install the rubber sleeve in the steering column paneling.

3. Install the lower steering column paneling.

• | Insert the ignition lock rosette.

Tighten
Tighten the 5 screws to 1 N·m (9 lb in).

• | Install the rubber sleeve in the steering column paneling.

4. Install the steering wheel. Refer to Steering Wheel Replacement.

Note: When replacing the control unit, before removing, carry out a Reset using the Tech 2. Refer to Control Module References.

5. Connect the battery.
6. For programming procedures, refer to Control Module References.