For 1990-2009 cars

# Seat Belt Latch Stop Button Available for Service

Subject: | Seat Belt Latch Stop Button Available for Service

Models: | 2005-2008 GM Passenger Cars and Light Duty Trucks (Including Saturn)

| 2005-2008 HUMMER H2

| 2006-2008 HUMMER H3

All seat belt retractor assemblies contain a stop button. If a stop button becomes damaged, the button can be replaced by ordering a replacement button through the GM Parts Catalog. The seat belt retractor assembly does not need replacement.

Refer to Document ID #1924486 in SI for the complete installation procedure.

### Parts Information

For part numbers, usage and availability of stop buttons, see Stop Kit in Group 14.875 (cars) or Group 16.714 (trucks) of the appropriate Parts Catalog. Saturn retailers should refer to the appropriate model year Parts & Illustration Catalog for the vehicle.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C9288 | Seat Belt Latch Stop Installation | Use Published Labor Operation Time