For 1990-2009 cars

## Instrument Panel Fuse Block 2009 G6

The instrument panel fuse block is located on the passenger side of the vehicle, on the lower portion of the instrument panel console near the floor.

Remove the console cover to access the fuse block, then remove the fuse block cover to access the fuses.

The vehicle may not be equipped with all the fuses and features listed.

Fuses | Usage
--- | ---
AIRBAG (BATT) | Airbag (Battery)
AIRBAG (IGN) | Airbag (Ignition)
CLUSTER/THEFT | Instrument Panel Cluster, Theft Deterrent System
DOOR LOCK | Door Locks
EPS | Electronic Power Steering
FUSE PULLER | Fuse Puller
HVAC BLOWER | Heating Ventilation Air Conditioning Blower Switch
HVAC BLOWER HIGH | Heating Ventilation Air Conditioning Blower - High Speed Relay
HVAC CTRL (BATT) | Heating Ventilation Air Conditioning Control Diagnostic Link Connector (Battery)
HVAC CTRL (IGN) | Heating Ventilation Air Conditioning Control (Ignition)
IGN SENSOR | Ignition Switch
INTERIOR LIGHTS | Interior Lamps
NOT INSTALLED | Not Used
NOT INSTALLED | Not Used
NOT INSTALLED | Not Used
NOT INSTALLED | Not Used
ONSTAR | OnStar®
PEDAL | Adjustable Pedals
POWER MIRRORS | Power Mirrors
POWER WINDOWS | Power Windows (Sedan)
RADIO | Audio System
ROOF/HEAT SEAT | Sunroof, Heated Seat, Power Windows (Coupe, Retractable Hardtop), Automatic Dimming Rearview Mirror, Compass
RUN/CRANK | Cruise Control Switch, Passenger Airbag Status Indicator, DSC Switch
SPARE FUSE HOLDER | Spare Fuse Holder
SPARE FUSE HOLDER | Spare Fuse Holder
SPARE FUSE HOLDER | Spare Fuse Holder
SPARE FUSE HOLDER | Spare Fuse Holder
STR/WHL ILLUM | Steering Wheel Controls Backlighting
WIPER SW | Windshield Wiper/Washer Switch