For 1990-2009 cars

#### Indicators

Symbol | Reference
--- | ---
| ABS: ABS Description and Operation
| Air Bag: SIR System Description and Operation
(CANADA) BRAKE | Brake: Hydraulic Brake System Description and Operation
| Charge: Charging System Description and Operation
| Door Ajar: Door Ajar Indicator Description and Operation
| Engine Coolant Temperature: Engine Coolant Temperature Indicator Malfunction
| Engine Oil Pressure: The IPC illuminates the engine oil pressure (EOP) indicator when the ECM detects the EOP is low from the EOP switch.
| Front Fog Lamps: Exterior Lighting Systems Description and Operation
| High Beam: Exterior Lighting Systems Description and Operation
| Low Fuel: Fuel System Description
| Low Oil Level: The IPC illuminates the low engine oil level indicator when the ECM detects the oil level is low from the engine oil level switch.
| MIL: Malfunction Indicator Lamp (MIL) Diagnosis
CANADA PASSENGER AIR BAG ON U.S | Passenger Air Bag: SIR System Description and Operation
| Rear Fog Lamps: Exterior Lighting Systems Description and Operation
| Seatbelt: Seat Belt System Description and Operation
| Security: Content Theft Deterrent (CTD) Description and Operation
| Service Vehicle Soon (SVS): The IPC illuminates this indicator when certain vehicle malfunctions that are not related to the emissions has occured
| Turn Signals: Exterior Lighting Systems Description and Operation
| Tow Haul: Transmission Component and System Description
| Tire Pressure Monitor (TPM): Tire Pressure Monitor Description and Operation
| Vehicle Stability Enhancement System (VSES): ABS Description and Operation