For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

The GMLAN modules on this vehicle also support DTC Symptom descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0012 | Driver Airbag Squib Circuit (Stage 1) | SDM | DTC B0012 or B0013
B0013 | Driver Airbag Squib Circuit (Stage 2) | SDM | DTC B0012 or B0013
B0014 | Driver Side Airbag Squib Circuit | SDM | DTC B0014-B0045
B0015 | Driver Pretensioner Circuit | SDM | DTC B0014-B0045
B0016 | Driver Curtain Airbag Squib Circuit | SDM | DTC B0014-B0045
B0019 | Passenger Airbag Squib Circuit (Stage 1) | SDM | DTC B0014-B0045
B0020 | Passenger Airbag Squib Circuit (Stage 2) | SDM | DTC B0014-B0045
B0021 | Passenger Side Airbag Squib Circuit | SDM | DTC B0014-B0045
B0022 | Passenger Pretensioner Circuit | SDM | DTC B0014-B0045
B0023 | Passenger Curtain Airbag Squib Circuit | SDM | DTC B0014-B0045
B004A | Door Unlock on Crash Relay Circuit Malfunction | UEC | DTC B004A
B0051 | Squib Circuits Activated (Crash) | SDM | DTC B0051, B0053, or B0055
B0052 | Passenger Airbag Locked By AOS (Automatic Occupancy Sensing) | SDM | DTC B0052, B0054, or B0058
B0053 | Deployment Commanded With Loop DTCs Present | SDM | DTC B0051, B0053, or B0055
B0054 | Passenger Side Airbag Locked By AOS (Automatic Occupancy Sensing) | SDM | DTC B0052, B0054, or B0058
B0055 | Deployment Side Airbag Deployment Commanded | SDM | DTC B0051, B0053, or B0055
B0058 | Passenger Pretensioner Locked By AOS (Automatic Occupancy Sensing) | SDM | DTC B0052, B0054, or B0058
B0080 | Passenger Seat Position Sensor | SDM | DTC B0080
B0081 | Replace AOS (Automatic Occupancy Sensing) | SDM | DTC B0081
B0083 | Left Or Middle EFS | SDM | DTC B0083-B0088
B0084 | Right EFS | SDM | DTC B0083-B0088
B0085 | Driver SIS | SDM | DTC B0083-B0088
B0086 | Passenger SIS | SDM | DTC B0083-B0088
B0158 | Outside Air Temperature (OAT) Sensor | UEC | DTC B0158
B0283 | Rear Window Heating Circuit Malfunction | REC | DTC B0283
B0525 | Front Right Turn Indicator Circuit Malfunction | UEC | DTC B0525 or B0530
B0530 | Front Left Turn Indicator Circuit Malfunction | UEC | DTC B0525 or B0530
B0655 | Center Brake Light Circuit | REC | DTC B0655
B0969 | Rear Window Heating Switch Telltale Circuit | IPC | DTC B0969
B1000 | Electronic Control Unit (ECU) Performance | IPC, Radio, REC, UEC, VCIM | DTC B1000
Trouble Code Memory Full | SDM | DTC B1000
B1001 | Option Configuration Error | IPC, Radio, REC, UEC, VCIM | DTC B1001
Electronic Control Unit (ECU) Not Programmed | SDM | DTC B1001
B1006 | Electronic Control Unit (ECU) Not Programmed | REC | DTC B1006
B1016 | VIN Not Programmed | REC, UEC | DTC B1016
B1019 | System Configuration Error | SDM | DTC B1019
B1020 | Rain Sensor | UEC | DTC B1020
B1023 | Key Stuck | Radio | DTC B1023
B1025 | Front Left Loudspeaker Circuit | Radio | DTC B1025-B1065
B1035 | Front Right Loudspeaker Circuit | Radio | DTC B1025-B1065
B1045 | Rear Left Loudspeaker Circuit | Radio | DTC B1025-B1065
B1055 | Rear Right Loudspeaker Circuit | Radio | DTC B1025-B1065
B1065 | Front Center Loudspeaker Circuit | Radio | DTC B1025-B1065
B1240 | CD Mechanism Malfunction | Radio | DTC B1240
B1245 | CD-Changer | Radio | DTC B1245-B1247 or B1249
B1246 | CD-Change Track Read Error | Radio | DTC B1245-B1247 or B1249
B1247 | CD-Change High Temperature | Radio | DTC B1245-B1247 or B1249
B1249 | CD-Change Table of Contents Read Error | Radio | DTC B1245-B1247 or B1249
B1272 | Antenna FM/AM Signal Circuit | Radio | DTC B1272
B1319 | Immobiliser Receiver Circuit | SCCM | DTC B1325
B1325 | Device Power 1 Circuit | SDM | DTC B1325
B1390 | Comfort Closing Circuit | REC | DTC B1390
B1428 | Starter Relay Malfunction | UEC | DTC B1428
B1446 | Replace Backup Power Source | VCIM | DTC B1446 or B1447
B1447 | Backup Power Source | VCIM | DTC B1446 or B1447
B1456 | Automatic Light Switch Circuit | IPC | DTC B1456
B2128 | Trip Reset Button Stuck | IPC | DTC B2128
B2455 | Cellular Phone Microphone Circuit Malfunction | VCIM | DTC B2455
B2470 | Cellular Phone Antenna Circuit Malfunction | VCIM | DTC B2470
B2476 | Cellular Phone Select Service Switch | VCIM | DTC B2476 or B2482
B2482 | Cellular Phone Select Switch Range/Performance | VCIM | DTC B2476 or B2482
B2483 | GPS Sensor Circuit Low | VCIM | DTC B2483 or B2484
B2484 | GPS Sensor Circuit Open | VCIM | DTC B2483 or B2484
B2501 | Horn Switch Stuck | SCCM | DTC B2501
B2530 | Front Fog Light Circuit | UEC | DTC B2530
B2545 | Rear Left Reverse Light Circuit | REC | DTC B2545 or B3880
B2570 | Trunk Lamp Circuit Malfunction | REC | DTC B2570
B2575 | Left Low Beam Circuit | UEC | DTC B2575 or B2699
B2580 | Left High Beam Circuit | UEC | DTC B2580 or B3866
B2585 | Front Left Parking Lamp Circuit | UEC | DTC B2585 or B3867
B2610 | Instrument Dimming Bulb Output Circuit | IPC | DTC B2610
B2652 | Inadvertent Load Circuit | REC | DTC B2652
B2662 | Parking Lamps Switch Circuit | IPC | DTC B2662
B2699 | Right Low Beam Circuit | UEC | DTC B2575 or B2699
B2740 | Front Fog Lights Switch | IPC | DTC B2740
B2961 | Ignition Key | SCCM | DTC B2961
B3055 | Transponder Key | SCCM | DTC B3055
B3056 | No Transponder Key Programmed | SCCM | DTC B3056
B3057 | Security Code Not Programmed | SCCM | DTC B3057
B3077 | Wrong Transponder Type Detected | SCCM | DTC B3077
B3109 | Remote-Key 1 System Voltage Low Voltage | SCCM | DTC B3109-B3113
B3110 | Remote-Key 2 System Voltage Low Voltage | SCCM | DTC B3109-B3113
B3111 | Remote-Key 3 System Voltage Low Voltage | SCCM | DTC B3109-B3113
B3112 | Remote-Key 4 System Voltage Low Voltage | SCCM | DTC B3109-B3113
B3113 | Remote-Key 5 System Voltage Low Voltage | SCCM | DTC B3109-B3113
B3114 | Remote-Key 1 Not Synchronized | SCCM | DTC B3114-B3118
B3115 | Remote-Key 2 Not Synchronized | SCCM | DTC B3114-B3118
B3116 | Remote-Key 3 Not Synchronized | SCCM | DTC B3114-B3118
B3117 | Remote-Key 4 Not Synchronized | SCCM | DTC B3114-B3118
B3118 | Remote-Key 5 Not Synchronized | SCCM | DTC B3114-B3118
B3130 | Doors Unlock Circuit Malfunction | REC | DTC B3130 or B3135
B3135 | Doors Lock Circuit Malfunction | REC | DTC B3130 or B3135
B3150 | Central Door Lock Switch | REC | DTC B3150
B3265 | Trunk Release Switch | REC | DTC B3265
B3596 | Hazard Warning Switch | IPC | DTC B3596
B3600 | Dimmed Illumination Switch Circuit | IPC | DTC B3600
B3634 | Left Turn Signal Switch | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B3635 | Right Turn Signal Switch | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B3636 | Left Turn Signal Switch | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B3637 | Rear Washer Switch | SCCM | DTC B3637-B3642
B3638 | Front Washer Switch | SCCM | DTC B3637-B3642
B3639 | Wiper Switch Up | SCCM | DTC B3637-B3642
B3640 | Wiper Switch Up | SCCM | DTC B3637-B3642
B3641 | Wiper Switch Down | SCCM | DTC B3637-B3642
B3642 | Wiper Switch Down | SCCM | DTC B3637-B3642
B3644 | Steering Wheel Remote Control Channel Up Switch | SCCM | DTC B3644
B3645 | Steering Wheel Remote Control Channel Down Switch | SCCM | DTC B3645
B3646 | Steering Wheel Scroll Wheel Right | SCCM | DTC B3646
B3647 | Steering Wheel Remote Control Voice Control Switch | SCCM | DTC B3647
B3648 | Steering Wheel Remote Control Phone Switch | SCCM | DTC B3648
B3649 | Steering Wheel Scroll Wheel Left | SCCM | DTC B3649
B3650 | Highbeam Switch | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B3651 | Headlamp Flasher Switch | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B3652 | Right Turn Signal Switch | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B370A | Rain Sensor Maifunction | UEC | DTC B370A
B3743 | Rear Window Heating Switch | IPC | DTC B3743
B3755 | No Transponder Key Programmed | SCCM | DTC B3755
B3794 | Cruise Control Select Switch | SCCM | DTC B3794
B3795 | Hazard Warning Switch Telltale | IPC | DTC B3795
B3803 | Windows Comfort Closing Circuit Malfunction | REC | DTC B3803
B3840 | Wrong Stalk Switch Configuration | SCCM | DTC B3634-B3636, B3650-B3652, or B3840
B3866 | Right High Beam Circuit | UEC | DTC B2580 or B3866
B3867 | Front Right Parking Lamp Circuit Malfunction | UEC | DTC B2585 or B3867
B3868 | Left Side Repeater Circuit Malfunction | UEC | DTC B3868 or B3869
B3869 | Right Side Repeater Circuit Malfunction | UEC | DTC B3868 or B3869
B3871 | Rear Side Markers Circuit Malfunction | REC | DTC B3871
B3874 | Wiper Low Speed Relay Circuit | UEC | DTC B3874
B3875 | Wiper High Speed Relay Circuit | UEC | DTC B3875
B3876 | Front Wiper Park Switch | UEC | DTC B3876
B3880 | Rear Right Reverse Light Circuit Malfunction | REC | DTC B2545 or B3880
B3883 | License Plate Light Circuit Malfunction | REC | DTC B3883
B3884 | Center Brake Light Circuit | REC | DTC B3884
B3899 | No Environment Identifier Learned | SCCM | DTC B3899
B3900 | No Immobiliser Identifier Learned | SCCM | DTC B3900
B3901 | Wrong Enviornment Identifier Received | SCCM | DTC B3901
B3902 | No Immobiliser Identifier Learned | SCCM | DTC B3902
B3909 | Low Beam Switch Circuit | IPC | DTC B3909
B3925 | Wrong Environment Identifier Received IPC | SCCM | DTC B3925, B3929, or B3977
B3929 | Wrong Environment Identifier Received REC | SCCM | DTC B3925, B3929, or B3977
B3977 | Wrong Environment Identifier Received UEC | SCCM | DTC B3925, B3929, or B3977
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0060 | Front Left Inlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0065 | Front Left Outlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0070 | Front Right Inlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0075 | Front Right Outlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0080 | Rear Left Inlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0085 | Rear Left Outlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0090 | Rear Right Inlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0095 | Rear Right Outlet Solenoid Valve Circuit Malfunction | EBCM | DTC C0060-C0095
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0121 | Valve Relay Circuit | EBCM | DTC C0121
C0131 | ABS Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Brake System (ABS) Brake Sensor Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer | EBCM | DTC C0186 or C0196
C0196 | Yaw Rate Circuit | EBCM | DTC C0186 or C0196
C0242 | Engine Control Module (ECM) Indicated TCS Malfunction | EBCM | DTC C0242 or P0856
C0252 | VSES Sensor | EBCM | DTC C0252
C0280 | Stability System Active Too Long | EBCM | DTC C0280
C0287 | Longitudinal Acceleration Sensor Circuit | EBCM | DTC C0287
C0292 | VSES Combination Sensor Circuits | EBCM | DTC C0292
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0558 | Tire Pressure Sensor IDs Not Learned | Tire Pressure Indicator Receiver | DTC C0558
C0569 | System Configuration Error | EBCM | DTC C0569
C0785 | One Undetermined Low Tire Pressure Sensor | Tire Pressure Indicator Receiver | DTC C0785-C0788
C0786 | Two Undetermined Low Tire Pressure Sensors | Tire Pressure Indicator Receiver | DTC C0785-C0788
C0787 | Three Undetermined Low Tire Pressure Sensors | Tire Pressure Indicator Receiver | DTC C0785-C0788
C0788 | Four Undetermined Low Tire Pressure Sensors | Tire Pressure Indicator Receiver | DTC C0785-C0788
C0800 | Device Power Circuit Voltage | EBCM | DTC C0800
C1508 | Internal Motor Circuit Malfunction | PSCM | DTC C1508
C1512 | Temperature Sensor Circuit | PSCM | DTC C1512
C1517 | Overheat Protection Mode Malfunction | PSCM | DTC C1517
C1523 | System Voltage | PSCM | DTC C1523
C1525 | Engine Running Signal | PSCM | DTC C1525
C1527 | Motor Circuit | PSCM | DTC C1527
C1528 | Motor Speed Invalid Signal Malfunction | PSCM | DTC C1528
C1529 | Motor Circuit | PSCM | DTC C1529
C1550 | ECU Failure | PSCM | DTC C1550
P000A | Intake Camshaft Position (CMP) System Slow Response | ECM | DTC P000A, P000B, P0011, or P0014
P000B | Exhaust Camshaft Position (CMP) System Slow Response | ECM | DTC P000A, P000B, P0011, or P0014
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010, P0013, or P2088-P2091
P0011 | Intake Camshaft Position (CMP) System Performance | ECM | DTC P000A, P000B, P0011, or P0014
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010, P0013, or P2088-P2091
P0014 | Exhaust Camshaft Position (CMP) System Performance | ECM | DTC P000A, P000B, P0011, or P0014
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068, P0121, or P0221
P0072 | Ambient Air Temperature (AAT) Sensor Circuit Low Voltage | ECM | DTC P0072-P0074
P0073 | Ambient Air Temperature (AAT) Sensor Circuit High Voltage | ECM | DTC P0072-P0074
P0074 | Ambient Air Temperature (AAT) Sensor Circuit Intermittent | ECM | DTC P0072-P0074
P009A | Intake Air Temperature (IAT)-Ambient Air Temperature (AAT) Correlation | ECM | DTC P009A
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101 or P1101
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Voltage | ECM | DTC P0102 or P0103
P0103 | Mass Air Flow (MAF) Sensor Circuit High Voltage | ECM | DTC P0102 or P0103
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0111
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0112, P0113, or P0114
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0112, P0113, or P0114
P0114 | Intake Air Temperature (IAT) Sensor Circuit Intermittent | ECM | DTC P0112, P0113, or P0114
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117, P0118, or P0119
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117, P0118, or P0119
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0117, P0118, or P0119
P0121 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0068, P0121, or P0221
Throttle Position (TP) Sensor Performance | TCM | DTC P0121, P0703, P0727, P1125, or P2637
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0128
P0130 | HO2S Circuit Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P0132 | HO2S Circuit High Voltage Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P0133 | HO2S Slow Response Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P0135 | HO2S Heater Performance Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0138 | HO2S Circuit High Voltage Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0139 | HO2S Circuit Slow Response Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0141 | HO2S Heater Performance Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0171 | Fuel Trim System Lean | ECM | DTC P0171 or P2096
P0172 | Fuel Trim System Rich | ECM | DTC P0172 or P2097
P0201 | Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0202 | Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0203 | Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0204 | Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0221 | Throttle Position (TP) Sensor 2 Performance | ECM | DTC P0068, P0121, or P0221
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0313 | Misfire Detected With Low Fuel Level | ECM | DTC P0300-P0304 or P0313
P0325 | Knock Sensor (KS) Circuit | ECM | DTC P0325 or P0326
P0326 | Knock Sensor (KS) Performance | ECM | DTC P0325 or P0326
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335 or P0336
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335 or P0336
P0340 | Intake Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340 or P0365
P0341 | Intake Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341 or P0366
P0365 | Exhaust Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340 or P0365
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341 or P0366
P0420 | Catalyst System Low Efficiency | ECM | DTC P0420
P0442 | Evaporative Emissions (EVAP) System Small Leak Detected | ECM | DTC P0442 or P0456
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0446 | Evaporative Emissions (EVAP) Vent System Performance | ECM | DTC P0446
P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451, P0452, P0453, or P0454
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0451, P0452, P0453, or P0454
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0451, P0452, P0453, or P0454
P0454 | Fuel Tank Pressure (FTP) Sensor Circuit Intermittent | ECM | DTC P0451, P0452, P0453, or P0454
P0455 | Evaporative Emission (EVAP) System Large Leak | ECM | DTC P0455
P0456 | Evaporative Emissions (EVAP) System Very Small Leak Detected | ECM | DTC P0442 or P0456
P0458 | Evaporative Emission (EVAP) Purge Solenoid Circuit Low Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0459 | Evaporative Emission (EVAP) Purge Solenoid Circuit High Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0460 | Fuel Level Sensor Range/Performance | ECM | DTC P0460
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Input | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Input | ECM | DTC P0463
P0464 | Fuel Level Sensor 1 Circuit Intermittent | ECM | DTC P0464
P0496 | Evaporative Emission System Flow During Non-Purge | ECM | DTC P0496
P0498 | Evaporative Emission (EVAP) Vent Solenoid Circuit Low Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Circuit High Voltage | ECM | DTC P0443, P0449, P0458, P0459, P0498, or P0499
P0500 | Vehicle Speed Signal Range/Performance | ECM | DTC P0500
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507
P0507 | Idle Speed High | ECM | DTC P0506 or P0507
P050A | Cold Start Idle Air Control System Performance | ECM | DTC P050A
P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM | DTC P0520
P0532 | Air Conditioning A/C Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning A/C Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0550 | Vehicle Odometer Information Invalid | ECM | DTC P0550
P0555 | Brake Booster Pressure Sensor Circuit | ECM | DTC P0555-P0558
P0558 | Brake Booster Pressure Sensor Circuit High Voltage | ECM | DTC P0555-P0558
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562 or P0563
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562 or P0563
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
Control Module Read Only Memory (ROM) | TCM | DTC P0601, P0603, or P0604
P0602 | Control Module Not Programmed | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P0603 | Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601, P0603, or P0604
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
Control Module Random Access Memory (RAM) | TCM | DTC P0601, P0603, or P0604
P0605 | Control Module Programming Read Only Memory (ROM) | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P0606 | Control Module Internal Performance | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P0607 | Control Module Performance | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P061A | Control Module Torque Performance | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P061B | Control Module Torque Calculation Performance | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P061C | Control Module Engine Speed Performance | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P0620 | Generator L-Terminal Circuit | ECM | DTC P0620
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0643 | 5-Volt Reference 1 Circuit High Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0646 | A/C Clutch Relay Control Circuit High | ECM | DTC P0646 or P0647
P0647 | A/C Clutch Relay Control Circuit Low | ECM | DTC P0646 or P0647
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0652 | 5-Volt Reference 2 Circuit Low Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0653 | 5-Volt Reference 2 Circuit High Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0654 | Engine Speed Signal Range/Performance | ECM | DTC P0654
P065E | Intake Manifold Tuning (IMT) Valve Performance | ECM | DTC P065E
P0661 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0661 or P0662
P0662 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit High Voltage | ECM | DTC P0661 or P0662
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0686, P0687, P0689, or P068B
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0686, P0687, P0689, or P068B
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0686, P0687, P0689, or P068B
P068B | Engine Controls Ignition Relay De-energized Too Late | ECM | DTC P0686, P0687, P0689, or P068B
P0691 | Fan Control 1 Circuit Low Voltage | ECM | DTC P0691-P0694
P0692 | Fan Control 1 Circuit High Voltage | ECM | DTC P0691-P0694
P0693 | Fan Control 2 Circuit Low Voltage | ECM | DTC P0691-P0694
P0694 | Fan Control 2 Circuit Low Voltage | ECM | DTC P0691-P0694
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700
P0703 | Brake Switch Circuit | ECM | DTC P0121, P0703, P0727, P1125, or P2637
P0705 | Transmission Range (TR) Switch Circuit | TCM | DTC P0705
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711, P0712, or P0713
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717 or P0722
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0717 or P0722
P0727 | Engine Speed No Signal | ECM | DTC P0121, P0703, P0727, P1125, or P2637
P0730 | Incorrect Gear Ratio | TCM | DTC P0730 or P0780
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM | DTC P0742
P0762 | Shift Solenoid (SS) 3 Valve Performance - Stuck On | TCM | DTC P0762, P079A, P07A2, or P07A3
P0780 | Incorrect Shift Pattern | TCM | DTC P0730 or P0780
P079A | Transmission Friction Element 1 Slip Detected | TCM | DTC P0762, P079A, P07A2, or P07A3
P07A2 | Transmission Friction Element 1 Performance | TCM | DTC P0762, P079A, P07A2, or P07A3
P07A3 | Transmission Friction Element 1 Stuck On | TCM | DTC P0762, P079A, P07A2, or P07A3
P0856 | Engine Control Module (ECM) Traction Control Torque Request Circuit | ECM | DTC C0242 or P0856
P0961 | Line Pressure Control (PC) Solenoid System Performance | TCM | DTC P0961-P0963 or P0965-P0967
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0961-P0963 or P0965-P0967
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0961-P0963 or P0965-P0967
P0965 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid System Performance | TCM | DTC P0961-P0963 or P0965-P0967
P0966 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0961-P0963 or P0965-P0967
P0967 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0961-P0963 or P0965-P0967
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, or P0980
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, or P0980
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, or P0980
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, or P0980
P0979 | Shift Solenoid (SS) 3 Control Circuit Low Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, or P0980
P0980 | Shift Solenoid (SS) 3 Control Circuit High Voltage | TCM | DTC P0973, P0974, P0976, P0977, P0979, or P0980
P1101 | Intake Air Flow System Performance | ECM | DTC P0101 or P1101
P1125 | Accelerator Pedal Position (APP) System | ECM | DTC P0121, P0703, P0727, P1125, or P2637
P1648 | Immobiliser Wrong Security Code | ECM | DTC P1648
P1649 | Immobiliser Security Code Not Programmed | ECM | DTC P1649
P1678 | Theft Deterrent System - Incorrect Enviornment Identification | ECM | DTC P1678 or P1679
P1679 | Theft Deterrent System - Incorrect Enviornment Identification | ECM | DTC P1678 or P1679
P2088 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2089 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2090 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2091 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit High Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2096 | Post Catalyst Fuel Trim System Low Limit | ECM | DTC P0171 or P2096
P2097 | Post Catalyst Fuel Trim System High Limit | ECM | DTC P0172 or P2097
P2100 | Throttle Actuator Control (TAC) Motor Control Circuit | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2101 | Throttle Actuator Position Performance | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2108 | Throttle Actuator Control (TAC) Module Performance | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2119 | Throttle Closed Position Performance | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2227, P2228, or P2229
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2227, P2228, or P2229
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P2297 | HO2S Performance During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P2301 | Ignition Coil 1 Control Circuit | ECM | DTC P2301, P2304, P2307, or P2310
P2304 | Ignition Coil 2 Control Circuit | ECM | DTC P2301, P2304, P2307, or P2310
P2307 | Ignition Coil 3 Control Circuit | ECM | DTC P2301, P2304, P2307, or P2310
P2310 | Ignition Coil 4 Control Circuit | ECM | DTC P2301, P2304, P2307, or P2310
P2500 | Generator L-Terminal Circuit Low Voltage | ECM | DTC P2500
P2544 | Transmission Torque Request Circuit | ECM | DTC P2544
P258C | Vacuum Pump Relay Control Circuit Low Voltage | ECM | DTC P258A-P258D
P258D | Vacuum Pump Relay Control Circuit High Voltage | ECM | DTC P258A-P258D
P2610 | Control Module Ignition OFF Timer Performance | ECM | DTC P0601-P0607, P061A, P061B, P061C, or P2610
P2637 | Transmission Torque Delivered Circuit | ECM | DTC P0121, P0703, P0727, P1125, or P2637
P2A00 | HO2S Performance Sensor 1 | ECM | DTC P0130-P0134, P2297, or P2A00
P2A01 | HO2S Performance Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
U1500 | Graphical Interface Communication Malfunction | IDM | DTC U1500
U2100 | Controller Area Network (CAN) Bus Communication | EBCM, ECM, IPC, Radio, REC, SCCM, SDM, TCM, UEC | DTC U2100
U2101 | Maximum Configuration List Not Programmed | EBCM, ECM, IPC, Radio, REC, SCCM, SDM, TCM, UEC | DTC U2101
U2105 | Lost Communication With Engine Control System | EBCM, IPC, REC, SCCM, TCM, UEC | DTC U2105-U2199
U2106 | Lost Communication With Transmission Control System | EBCM, ECM, SCCM | DTC U2105-U2199
U2107 | Lost Communication With Body Control System | EBCM, ECM, IPC, PSCM, SCCM, REC, SDM, TCM, UEC | DTC U2105-U2199
U2108 | Lost Communication With ABS/TCS Control System | ECM, IPC, SCCM, REC, TCM, UEC | DTC U2105-U2199
U2109 | Lost Communication With ABS/TCS Control System | ECM, IPC, SCCM, REC, TCM, UEC | DTC U2105-U2199
U2111 | Lost Communication With Steering Control System | SCCM | DTC U2105-U2199
U2113 | Lost Communication With Sensing and Diagnostic Module (SDM) | IPC, SCCM | DTC U2105-U2199
U2116 | Lost Communication With Instrument Panel Cluster (IPC) | PSCM, REC, SCCM, SDM, UEC | DTC U2105-U2199
U2201 | Lost Communication With Electronic Head Unit (EHU) | DIC | DTC U2201