For 1990-2009 cars

Warning: Refer to Brake Dust Warning in the Preface section.

1. Remove brake linings. Refer to Front Disc Brake Pads Replacement or Rear Disc Brake Pads Replacement.
2. Measure the remaining brake lining thickness with a caliper (1).
3. Nominal values. Refer to Disc Brake Component Specifications.
4. Install brake pads.
5. Install the brake linings. Refer to Front Disc Brake Pads Replacement or Rear Disc Brake Pads Replacement.