For 1990-2009 cars

The equipment you will need is located in the rear storage area.

1. Open the liftgate. See Liftgate.
2. Lift the floor cover to access the spare tire and tools.
3. Remove the foam pad. Turn the retainer counterclockwise to remove it.
4. Remove the spare tire by pulling it up and out of the trunk.
5. The jack and tools are stored below the spare tire.
6. The tools you will be using include the jack (A), wheel wrench (B), screwdriver (C), and jack handle (D).