For 1990-2009 cars

Note: The front differential transfer drive gear assembly (14) is non-serviciable and replaced as an assembly.

1. Remove the front differential transfer drive gear assembly (14).
2. Remove the front differential transfer drive gear front thrust bearing race (263) from the front differential transfer drive gear assembly (14).
3. Remove the front differential transfer drive gear rear thrust bearing assembly (270) and front differential transfer drive gear rear thrust bearing race (269).