For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Active Head Restraint Frame Bolts | 3.5 N·m | 32 lb in
Bracket Bolts - Left and Right | 25 N·m | 18 lb ft
Exterior Paneling Bolts | 35 N·m | 26 lb ft
Front Seat Backrest Bolts | 35 N·m | 26 lb ft
Front Seat Backrest Trim Bolts | 3 N·m | 26 lb in
Front Seat Belt Bolt | 20 N·m | 15 lb ft
Front Seat Rear Bolts | 35 N·m | 26 lb ft
Front Seat Seat Belt Bolt | 25 N·m | 18 lb ft
Interior Paneling Bolt | 2.5 N·m | 22 lb in
Lock Panel Bolts | 25 N·m | 18 lb ft
Molding Bolts - Left and Right | 2.5 N·m | 22 lb in
Rear Seat Back Bolts | 20 N·m | 15 lb ft
Rear Seat Back Cushion Bolts | 42 N·m | 32 lb ft
Rear Seat Back Cushion Bolts - Side | 20 N·m | 15 lb ft
Rear Seat Back Cushion Latch Bolts | 25 N·m | 18 lb ft
Rear Seat Back Cushion Latch Striker | 60 N·m | 44 lb ft
Rear Seat Back Cushion Screw - Back | 20 N·m | 15 lb ft
Rear Seat Backrest Seat Belt Buckle Bolts - Front | 20 N·m | 15 lb ft
Rear Seat Backrest Seat Belt Buckle Bolts - Side | 20 N·m | 15 lb ft
Rear Seat Backrest Bolts - Side | 20 N·m | 15 lb ft
Rear Seat Backrest Screws - Back | 20 N·m | 15 lb ft
Seat Back Cushion Pad Support Bolt | 3 N·m | 26 lb in
Seat Belt Bolt | 35 N·m | 26 lb ft
Seat Belt Buckle Bolts | 20 N·m | 15 lb ft
Seat Belt Buckle Front Screw | 20 N·m | 15 lb ft
Seat Belt Buckle Tensioner in Bracket Bolt | 35 N·m | 26 lb ft
Seat Belt Lock Bolt | 35 N·m | 26 lb ft
Seat Belt to Front Seat Bolt | 20 N·m | 15 lb ft
Seat Height Adjuster Bolts | 35 N·m | 26 lb ft
Side Airbag Bolts | 5 N·m | 44 lb in