For 1990-2009 cars

Condition | Action
--- | ---
DEFINITION: Harsh feel without causing an upshift or downshift. Concern is most noticeable with light acceleration or deceleration.
Engine or transmission mounts |

• | Inspect the engine mounts and the transmission mounts for wear or loose mounting fasteners.

• | Replace any faulty engine or transmission mounts or loose fasteners.

Engine malfunction |

• | Ensure engine is operating properly.

• | Repair engine to operate properly.

Drive shafts |

• | Inspect the drive shafts for worn components.

• | Replace the drive shaft if worn.

Suspension system |

• | Inspect suspension components.

• | Replace faulty suspension components.