For 1990-2009 cars

#### Transmission Fluid

Transmission | Filling quantity | GM Part Number | Canadian
--- | --- | --- | ---
F17+ F17+ MTA | Approx. 1.60 L (1.69 qt) | 88862472 | 88862473
Transmission Fluid Level: All transmissions, after a transmission repair, should be filled as far as the lower edge of the inspection aperture. The transmission fluid is supplied by weight in production. There is no need to correct it during scheduled servicing if no leaks are found.